Filetype: IR signals file
Version: 1
#
name: 0
type: parsed
protocol: NECext
address: 87 5E 00 00
command: 00 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 87 5E 00 00
command: 01 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 87 5E 00 00
command: 02 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 87 5E 00 00
command: 03 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 87 5E 00 00
command: 04 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 87 5E 00 00
command: 05 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 87 5E 00 00
command: 06 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 87 5E 00 00
command: 07 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 87 5E 00 00
command: 08 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 87 5E 00 00
command: 09 00 00 00
#
name: Key
type: parsed
protocol: NECext
address: 87 5E 00 00
command: 0A 00 00 00
#
name: UP
type: parsed
protocol: NECext
address: 87 5E 00 00
command: 0B 00 00 00
#
name: DOWN
type: parsed
protocol: NECext
address: 87 5E 00 00
command: 0C 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 87 5E 00 00
command: 0D 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 87 5E 00 00
command: 0E 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 87 5E 00 00
command: 0F 00 00 00
#
name: CHANNELUP
type: parsed
protocol: NECext
address: 87 5E 00 00
command: 10 00 00 00
#
name: Q
type: parsed
protocol: NECext
address: 87 5E 00 00
command: 11 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 87 5E 00 00
command: 12 00 00 00
#
name: Head
type: parsed
protocol: NECext
address: 87 5E 00 00
command: 13 00 00 00
#
name: R
type: parsed
protocol: NECext
address: 87 5E 00 00
command: 14 00 00 00
#
name: OK
type: parsed
protocol: NECext
address: 87 5E 00 00
command: 15 00 00 00
#
name: Red_A
type: parsed
protocol: NECext
address: 87 5E 00 00
command: 16 00 00 00
#
name: Green_B
type: parsed
protocol: NECext
address: 87 5E 00 00
command: 17 00 00 00
#
name: Yellow_C
type: parsed
protocol: NECext
address: 87 5E 00 00
command: 18 00 00 00
#
name: Blue_D
type: parsed
protocol: NECext
address: 87 5E 00 00
command: 19 00 00 00
#
name: CHANNELDOWN
type: parsed
protocol: NECext
address: 87 5E 00 00
command: 1A 00 00 00
#
name: LEFT
type: parsed
protocol: NECext
address: 87 5E 00 00
command: 1B 00 00 00
#
name: RIGHT
type: parsed
protocol: NECext
address: 87 5E 00 00
command: 1C 00 00 00
#
name: TEXT
type: parsed
protocol: NECext
address: 87 5E 00 00
command: 1D 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 87 5E 00 00
command: 1E 00 00 00
#
name: Swap
type: parsed
protocol: NECext
address: 87 5E 00 00
command: 1F 00 00 00
#
name: Interface
type: parsed
protocol: NECext
address: 87 5E 00 00
command: 20 00 00 00
#
name: Tone
type: parsed
protocol: NECext
address: 87 5E 00 00
command: 21 00 00 00
#
name: I
type: parsed
protocol: NECext
address: 87 5E 00 00
command: 24 00 00 00
#
name: Navigator
type: parsed
protocol: NECext
address: 87 5E 00 00
command: 25 00 00 00
#
name: RightArr
type: parsed
protocol: NECext
address: 87 5E 00 00
command: 26 00 00 00
#
name: LeftArr
type: parsed
protocol: NECext
address: 87 5E 00 00
command: 28 00 00 00
