Filetype: IR signals file
Version: 1
#
name: 0
type: parsed
protocol: NECext
address: B6 00 00 00
command: 00 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: B6 00 00 00
command: 01 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: B6 00 00 00
command: 02 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: B6 00 00 00
command: 03 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: B6 00 00 00
command: 04 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: B6 00 00 00
command: 05 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: B6 00 00 00
command: 06 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: B6 00 00 00
command: 07 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: B6 00 00 00
command: 08 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: B6 00 00 00
command: 09 00 00 00
#
name: 10CHANNELSUP
type: parsed
protocol: NECext
address: B6 00 00 00
command: 0A 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: B6 00 00 00
command: 11 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: B6 00 00 00
command: 13 00 00 00
#
name: BACK
type: parsed
protocol: NECext
address: B6 00 00 00
command: 14 00 00 00
#
name: FORWARD
type: parsed
protocol: NECext
address: B6 00 00 00
command: 15 00 00 00
#
name: LAST
type: parsed
protocol: NECext
address: B6 00 00 00
command: 16 00 00 00
#
name: NEXT
type: parsed
protocol: NECext
address: B6 00 00 00
command: 17 00 00 00
#
name: CLEAR
type: parsed
protocol: NECext
address: B6 00 00 00
command: 1A 00 00 00
#
name: check
type: parsed
protocol: NECext
address: B6 00 00 00
command: 1B 00 00 00
#
name: p.mode
type: parsed
protocol: NECext
address: B6 00 00 00
command: 1F 00 00 00
#
name: SPACE
type: parsed
protocol: NECext
address: B6 00 00 00
command: 42 00 00 00
#
name: AGAIN
type: parsed
protocol: NECext
address: B6 00 00 00
command: 43 00 00 00
#
name: DOWN
type: parsed
protocol: NECext
address: B6 00 00 00
command: 48 00 00 00
#
name: UP
type: parsed
protocol: NECext
address: B6 00 00 00
command: 49 00 00 00
#
name: EDIT
type: parsed
protocol: NECext
address: B6 00 00 00
command: 4A 00 00 00
#
name: random
type: parsed
protocol: NECext
address: B6 00 00 00
command: 4F 00 00 00
#
name: peak_search
type: parsed
protocol: NECext
address: B6 00 00 00
command: 8D 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: B6 00 00 00
command: 91 00 00 00
