Filetype: IR signals file
Version: 1
#
name: 8
type: parsed
protocol: NECext
address: 50 00 00 00
command: 04 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 50 00 00 00
command: 05 00 00 00
#
name: AV
type: parsed
protocol: NECext
address: 50 00 00 00
command: 09 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 50 00 00 00
command: 0B 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 50 00 00 00
command: 0C 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 50 00 00 00
command: 0D 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 50 00 00 00
command: 0E 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 50 00 00 00
command: 0F 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 50 00 00 00
command: 12 00 00 00
#
name: CH
type: parsed
protocol: NECext
address: 50 00 00 00
command: 13 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 50 00 00 00
command: 15 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 50 00 00 00
command: 17 00 00 00
#
name: CHANNELDOWN
type: parsed
protocol: NECext
address: 50 00 00 00
command: 18 00 00 00
#
name: CHANNELUP
type: parsed
protocol: NECext
address: 50 00 00 00
command: 19 00 00 00
#
name: HELP
type: parsed
protocol: NECext
address: 50 00 00 00
command: 1A 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 50 00 00 00
command: 1C 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 50 00 00 00
command: 1D 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 50 00 00 00
command: 1E 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 50 00 00 00
command: 1F 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 50 00 00 00
command: 40 00 00 00
#
name: OK
type: parsed
protocol: NECext
address: 50 00 00 00
command: 43 00 00 00
#
name: PSCAN100HZ
type: parsed
protocol: NECext
address: 50 00 00 00
command: 4D 00 00 00
#
name: X
type: parsed
protocol: NECext
address: 50 00 00 00
command: 54 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 50 00 00 00
command: 5F 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 50 00 00 00
command: 6B 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 50 00 00 00
command: 6C 00 00 00
#
name: REV
type: parsed
protocol: NECext
address: 50 00 00 00
command: 6D 00 00 00
#
name: FORWARD
type: parsed
protocol: NECext
address: 50 00 00 00
command: 6F 00 00 00
