Filetype: IR signals file
Version: 1
# 
# Hisense TV ZDB2190126
#
name: POWER
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 0D F2 00 00
# 
name: VOL+
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 44 BB 00 00
# 
name: VOL-
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 43 BC 00 00
# 
name: Ok
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 15 EA 00 00
# 
name: Up
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 16 E9 00 00
# 
name: Down
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 17 E8 00 00
# 
name: Left
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 19 E6 00 00
# 
name: Right
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 18 E7 00 00
# 
name: MUTE
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 0E F1 00 00
# 
name: CH+
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 4A B5 00 00
# 
name: CH-
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 4B B4 00 00
# 
name: Home
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 20 DF 00 00
# 
name: Back
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 48 B7 00 00
# 
name: Exit
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 5C A3 00 00
# 
name: Input
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 12 ED 00 00
# 
name: Youtube
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 5A A5 00 00
