Filetype: IR signals file
Version: 1
#
name: 1
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 00 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 01 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 02 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 03 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 04 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 05 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 06 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 07 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 08 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 09 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 09 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 09 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 09 00 00 00
#
name: >25
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 0A 00 00 00
#
name: ENTER
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 0B 00 00 00
#
name: CHECK
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 0D 00 00 00
#
name: UNK4
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 0D 00 00 00
#
name: CLEAR
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 0F 00 00 00
#
name: CLEAR
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 0F 00 00 00
#
name: UNK6
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 0F 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 12 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 13 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 15 00 00 00
#
name: EJECTCD
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 16 00 00 00
#
name: DISPLAY
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 18 00 00 00
#
name: SCROLL
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 19 00 00 00
#
name: NONAME2
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 1A 00 00 00
#
name: NONAME1
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 1B 00 00 00
#
name: CONTINUE
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 1D 00 00 00
#
name: SHUFFLE
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 1E 00 00 00
#
name: PROGRAM
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 1F 00 00 00
#
name: PREVIOUS
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 20 00 00 00
#
name: NEXT
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 21 00 00 00
#
name: AGAIN
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 26 00 00 00
#
name: A-B
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 27 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 28 00 00 00
#
name: MEMO
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 28 00 00 00
#
name: PAUSE
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 29 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 2A 00 00 00
#
name: REWIND
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 2B 00 00 00
#
name: FORWARD
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 2C 00 00 00
#
name: AGAIN
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 2C 00 00 00
#
name: RECORD
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 2D 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 2E 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 2F 00 00 00
#
name: T.REC
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 30 00 00 00
#
name: PREVIOUS
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 30 00 00 00
#
name: NEXT
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 31 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 32 00 00 00
#
name: AUTO_SPACE
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 33 00 00 00
#
name: REWIND
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 33 00 00 00
#
name: MUSIC_SCAN
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 34 00 00 00
#
name: FORWARD
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 34 00 00 00
#
name: WRITE_CHAR
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 36 00 00 00
#
name: WRITE_NUM
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 37 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 38 00 00 00
#
name: PAUSE
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 39 00 00 00
#
name: WRITE_NAME
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 3C 00 00 00
#
name: KPMINUS
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 3D 00 00 00
#
name: SLEEP
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 3E 00 00 00
#
name: KPPLUS
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 3E 00 00 00
#
name: MUSIC_SYNC
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 3F 00 00 00
#
name: EXTRA
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 3F 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 40 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 41 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 42 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 43 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 44 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 45 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 46 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 47 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 48 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 49 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 4A 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 4B 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 4C 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 4D 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 4E 00 00 00
#
name: FADE
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 5F 00 00 00
#
name: JOG+
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 60 00 00 00
#
name: JOG-
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 61 00 00 00
#
name: JOG++
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 62 00 00 00
#
name: UNK2
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 62 00 00 00
#
name: UNK5
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 63 00 00 00
#
name: JOG+++
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 64 00 00 00
#
name: UNK1
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 64 00 00 00
#
name: UNK3
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 65 00 00 00
#
name: MEMO_INPUT
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 69 00 00 00
#
name: MEMO_SCAN
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 6B 00 00 00
