Filetype: IR signals file
Version: 1
#
name: 1
type: parsed
protocol: NECext
address: 02 00 00 00
command: 00 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 02 00 00 00
command: 01 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 02 00 00 00
command: 02 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 02 00 00 00
command: 03 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 02 00 00 00
command: 04 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 02 00 00 00
command: 05 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 02 00 00 00
command: 06 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 02 00 00 00
command: 07 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 02 00 00 00
command: 08 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 02 00 00 00
command: 09 00 00 00
#
name: ENTER
type: parsed
protocol: NECext
address: 02 00 00 00
command: 0B 00 00 00
#
name: CHANNELUP
type: parsed
protocol: NECext
address: 02 00 00 00
command: 10 00 00 00
#
name: CHANNELDOWN
type: parsed
protocol: NECext
address: 02 00 00 00
command: 11 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 02 00 00 00
command: 12 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 02 00 00 00
command: 13 00 00 00
#
name: JOG_2_SPEED
type: parsed
protocol: NECext
address: 02 00 00 00
command: 14 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 02 00 00 00
command: 15 00 00 00
#
name: RESET
type: parsed
protocol: NECext
address: 02 00 00 00
command: 16 00 00 00
#
name: AUDIO_MONITOR
type: parsed
protocol: NECext
address: 02 00 00 00
command: 17 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 02 00 00 00
command: 18 00 00 00
#
name: PAUSE
type: parsed
protocol: NECext
address: 02 00 00 00
command: 19 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 02 00 00 00
command: 1A 00 00 00
#
name: COLOR-
type: parsed
protocol: NECext
address: 02 00 00 00
command: 1B 00 00 00
#
name: RECORD
type: parsed
protocol: NECext
address: 02 00 00 00
command: 1D 00 00 00
#
name: BRIGHT+
type: parsed
protocol: NECext
address: 02 00 00 00
command: 1E 00 00 00
#
name: BRIGHT-
type: parsed
protocol: NECext
address: 02 00 00 00
command: 1F 00 00 00
#
name: HUE+
type: parsed
protocol: NECext
address: 02 00 00 00
command: 20 00 00 00
#
name: HUE-
type: parsed
protocol: NECext
address: 02 00 00 00
command: 21 00 00 00
#
name: SHARP+
type: parsed
protocol: NECext
address: 02 00 00 00
command: 22 00 00 00
#
name: JOG_1/5_SPEED
type: parsed
protocol: NECext
address: 02 00 00 00
command: 23 00 00 00
#
name: TUNER
type: parsed
protocol: NECext
address: 02 00 00 00
command: 24 00 00 00
#
name: TV/VIDEO
type: parsed
protocol: NECext
address: 02 00 00 00
command: 25 00 00 00
#
name: BAL_LEFT
type: parsed
protocol: NECext
address: 02 00 00 00
command: 26 00 00 00
#
name: BAL_RIGHT
type: parsed
protocol: NECext
address: 02 00 00 00
command: 27 00 00 00
#
name: SEARCH-
type: parsed
protocol: NECext
address: 02 00 00 00
command: 28 00 00 00
#
name: SEARCH+
type: parsed
protocol: NECext
address: 02 00 00 00
command: 29 00 00 00
#
name: ANT/VCR
type: parsed
protocol: NECext
address: 02 00 00 00
command: 2A 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 02 00 00 00
command: 2E 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 02 00 00 00
command: 2F 00 00 00
#
name: JOG-
type: parsed
protocol: NECext
address: 02 00 00 00
command: 30 00 00 00
#
name: JOG+
type: parsed
protocol: NECext
address: 02 00 00 00
command: 31 00 00 00
#
name: JOG_1_SPEED
type: parsed
protocol: NECext
address: 02 00 00 00
command: 33 00 00 00
#
name: SLEEP
type: parsed
protocol: NECext
address: 02 00 00 00
command: 36 00 00 00
#
name: CHANNELDOWN
type: parsed
protocol: NECext
address: 02 00 00 00
command: 3A 00 00 00
#
name: JUMP
type: parsed
protocol: NECext
address: 02 00 00 00
command: 3B 00 00 00
#
name: SLOW+
type: parsed
protocol: NECext
address: 02 00 00 00
command: 3D 00 00 00
#
name: SLOW-
type: parsed
protocol: NECext
address: 02 00 00 00
command: 3E 00 00 00
#
name: INPUT1
type: parsed
protocol: NECext
address: 02 00 00 00
command: 40 00 00 00
#
name: INPUT2
type: parsed
protocol: NECext
address: 02 00 00 00
command: 41 00 00 00
#
name: CURSOR_UP
type: parsed
protocol: NECext
address: 02 00 00 00
command: 42 00 00 00
#
name: CURSOR_DOWN
type: parsed
protocol: NECext
address: 02 00 00 00
command: 43 00 00 00
#
name: INPUT5
type: parsed
protocol: NECext
address: 02 00 00 00
command: 44 00 00 00
#
name: INPUT6
type: parsed
protocol: NECext
address: 02 00 00 00
command: 45 00 00 00
#
name: COUNTER_RESET
type: parsed
protocol: NECext
address: 02 00 00 00
command: 46 00 00 00
#
name: INPUT8
type: parsed
protocol: NECext
address: 02 00 00 00
command: 47 00 00 00
#
name: INDEX_MARK
type: parsed
protocol: NECext
address: 02 00 00 00
command: 48 00 00 00
#
name: INDEX_ERASE
type: parsed
protocol: NECext
address: 02 00 00 00
command: 49 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 02 00 00 00
command: 4D 00 00 00
#
name: CABLE
type: parsed
protocol: NECext
address: 02 00 00 00
command: 4E 00 00 00
#
name: INPUT_SELECT
type: parsed
protocol: NECext
address: 02 00 00 00
command: 4F 00 00 00
#
name: EXECUTE
type: parsed
protocol: NECext
address: 02 00 00 00
command: 51 00 00 00
#
name: INDEX
type: parsed
protocol: NECext
address: 02 00 00 00
command: 53 00 00 00
#
name: RECORD
type: parsed
protocol: NECext
address: 02 00 00 00
command: 58 00 00 00
#
name: DATA_SCREEN
type: parsed
protocol: NECext
address: 02 00 00 00
command: 5A 00 00 00
#
name: NEXT
type: parsed
protocol: NECext
address: 02 00 00 00
command: 5D 00 00 00
#
name: INFO
type: parsed
protocol: NECext
address: 02 00 00 00
command: 60 00 00 00
#
name: CURSOR_RIGHT
type: parsed
protocol: NECext
address: 02 00 00 00
command: 61 00 00 00
#
name: CURSOR_LEFT
type: parsed
protocol: NECext
address: 02 00 00 00
command: 62 00 00 00
#
name: TIMER_CLEAR
type: parsed
protocol: NECext
address: 02 00 00 00
command: 63 00 00 00
#
name: ASC
type: parsed
protocol: NECext
address: 02 00 00 00
command: 64 00 00 00
#
name: TIMER_ON/OFF
type: parsed
protocol: NECext
address: 02 00 00 00
command: 65 00 00 00
#
name: AUTOPROG
type: parsed
protocol: NECext
address: 02 00 00 00
command: 68 00 00 00
#
name: CH_AUTO_PGM
type: parsed
protocol: NECext
address: 02 00 00 00
command: 6B 00 00 00
#
name: AV+
type: parsed
protocol: NECext
address: 02 00 00 00
command: 74 00 00 00
#
name: AV-
type: parsed
protocol: NECext
address: 02 00 00 00
command: 75 00 00 00
#
name: CH_ADD
type: parsed
protocol: NECext
address: 02 00 00 00
command: 78 00 00 00
#
name: CH_DEL
type: parsed
protocol: NECext
address: 02 00 00 00
command: 79 00 00 00
#
name: HIGH_SPEED_REWIND
type: parsed
protocol: NECext
address: 02 00 00 00
command: 7D 00 00 00
#
name: JOG_END
type: parsed
protocol: NECext
address: 02 00 00 00
command: 7E 00 00 00
