Filetype: IR signals file
Version: 1
# 
# Samsung AA59-00741A TV
# by sealldeveloper
#
name: POWER
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 02 00 00 00
# 
name: VOL+
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 07 00 00 00
# 
name: VOL-
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 0B 00 00 00
# 
name: MUTE
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 0F 00 00 00
# 
name: CH+
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 12 00 00 00
# 
name: CH-
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 12 00 00 00
# 
name: ChList
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 6B 00 00 00
# 
name: TTX/MIX
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 6B 00 00 00
# 
name: Source
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 6B 00 00 00
# 
name: PreCh
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 13 00 00 00
# 
name: MediaP
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 8C 00 00 00
# 
name: Menu
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 1A 00 00 00
# 
name: Guide
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 4F 00 00 00
# 
name: Info
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 1F 00 00 00
# 
name: Up
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 60 00 00 00
# 
name: Left
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 60 00 00 00
# 
name: Right
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 60 00 00 00
# 
name: Down
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 60 00 00 00
# 
name: Ctr
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 60 00 00 00
# 
name: Tools
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 4B 00 00 00
# 
name: Return
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 58 00 00 00
# 
name: Exit
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 2D 00 00 00
# 
name: Red/A
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 6C 00 00 00
# 
name: Green/B
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 14 00 00 00
# 
name: Yellow/C
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 15 00 00 00
# 
name: Blue/D
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 16 00 00 00
# 
name: Emanual
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 3F 00 00 00
# 
name: PSize
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 3E 00 00 00
# 
name: Ad/Subt.
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 25 00 00 00
# 
name: Stop
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 46 00 00 00
# 
name: Rewind
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 45 00 00 00
# 
name: Play
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 47 00 00 00
# 
name: Pause
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 4A 00 00 00
# 
name: FastForward
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 48 00 00 00
# 
name: 0
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 11 00 00 00
# 
name: 1
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 04 00 00 00
# 
name: 2
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 05 00 00 00
# 
name: 3
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 06 00 00 00
# 
name: 4
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 08 00 00 00
# 
name: 5
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 09 00 00 00
# 
name: 6
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 0A 00 00 00
# 
name: 7
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 0C 00 00 00
# 
name: 8
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 0D 00 00 00
# 
name: 9
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 0E 00 00 00
