Filetype: IR signals file
Version: 1
#
name: 0
type: parsed
protocol: NECext
address: 00 00 00 00
command: 00 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 00 00 00 00
command: 01 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 00 00 00 00
command: 02 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 00 00 00 00
command: 03 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 00 00 00 00
command: 04 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 00 00 00 00
command: 05 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 00 00 00 00
command: 06 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 00 00 00 00
command: 07 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 00 00 00 00
command: 08 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 00 00 00 00
command: 09 00 00 00
#
name: EMPTY_BUTTON
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0A 00 00 00
#
name: _/__
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0B 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0C 00 00 00
#
name: OK
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0D 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0E 00 00 00
#
name: WIN+
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0F 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 00 00 00 00
command: 10 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 00 00 00 00
command: 11 00 00 00
#
name: ZOOMIN
type: parsed
protocol: NECext
address: 00 00 00 00
command: 14 00 00 00
#
name: ZOOMOUT
type: parsed
protocol: NECext
address: 00 00 00 00
command: 15 00 00 00
#
name: BLUE
type: parsed
protocol: NECext
address: 00 00 00 00
command: 1E 00 00 00
#
name: CHANNELUP
type: parsed
protocol: NECext
address: 00 00 00 00
command: 20 00 00 00
#
name: CHANNELDOWN
type: parsed
protocol: NECext
address: 00 00 00 00
command: 21 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 00 00 00 00
command: 23 00 00 00
#
name: PAUSE
type: parsed
protocol: NECext
address: 00 00 00 00
command: 24 00 00 00
#
name: POINT
type: parsed
protocol: NECext
address: 00 00 00 00
command: 29 00 00 00
#
name: YELLOW
type: parsed
protocol: NECext
address: 00 00 00 00
command: 2B 00 00 00
#
name: GREEN
type: parsed
protocol: NECext
address: 00 00 00 00
command: 2C 00 00 00
#
name: RED
type: parsed
protocol: NECext
address: 00 00 00 00
command: 2D 00 00 00
#
name: EXIT
type: parsed
protocol: NECext
address: 00 00 00 00
command: 2E 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 00 00 00 00
command: 32 00 00 00
#
name: FORWARD
type: parsed
protocol: NECext
address: 00 00 00 00
command: 34 00 00 00
#
name: GRAY
type: parsed
protocol: NECext
address: 00 00 00 00
command: 35 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 00 00 00 00
command: 36 00 00 00
#
name: REWIND
type: parsed
protocol: NECext
address: 00 00 00 00
command: 37 00 00 00
#
name: AV
type: parsed
protocol: NECext
address: 00 00 00 00
command: 38 00 00 00
#
name: WIN_IN
type: parsed
protocol: NECext
address: 00 00 00 00
command: 39 00 00 00
#
name: LINES_WIN
type: parsed
protocol: NECext
address: 00 00 00 00
command: 3C 00 00 00
#
name: MINIMIZE
type: parsed
protocol: NECext
address: 00 00 00 00
command: 3E 00 00 00
#
name: F11
type: parsed
protocol: NECext
address: 00 00 00 00
command: 3F 00 00 00
