Filetype: IR signals file
Version: 1
# 
name: POWER
type: parsed
protocol: NECext
address: 30 FC 00 00
command: 10 EF 00 00
# 
name: Eject
type: parsed
protocol: NECext
address: 30 FC 00 00
command: 4A B5 00 00
# 
name: Mode
type: parsed
protocol: NECext
address: 30 FC 00 00
command: 06 F9 00 00
# 
name: Menu
type: parsed
protocol: NECext
address: 30 FC 00 00
command: 18 E7 00 00
# 
name: Moon ZZZ
type: parsed
protocol: NECext
address: 30 FC 00 00
command: 03 FC 00 00
# 
name: Snooze
type: parsed
protocol: NECext
address: 30 FC 00 00
command: 07 F8 00 00
# 
name: BT Pair
type: parsed
protocol: NECext
address: 30 FC 00 00
command: 58 A7 00 00
# 
name: Alarm 1
type: parsed
protocol: NECext
address: 30 FC 00 00
command: 47 B8 00 00
# 
name: Alarm 2
type: parsed
protocol: NECext
address: 30 FC 00 00
command: 57 A8 00 00
# 
name: Dimmer
type: parsed
protocol: NECext
address: 30 FC 00 00
command: 01 FE 00 00
# 
name: Play_Pause
type: parsed
protocol: NECext
address: 30 FC 00 00
command: 02 FD 00 00
# 
name: Stop
type: parsed
protocol: NECext
address: 30 FC 00 00
command: 05 FA 00 00
# 
name: Folder Down
type: parsed
protocol: NECext
address: 30 FC 00 00
command: 14 EB 00 00
# 
name: Folder Up
type: parsed
protocol: NECext
address: 30 FC 00 00
command: 0F F0 00 00
# 
name: Skip Backwards
type: parsed
protocol: NECext
address: 30 FC 00 00
command: 11 EE 00 00
# 
name: Fast Backwards
type: parsed
protocol: NECext
address: 30 FC 00 00
command: 0A F5 00 00
# 
name: Fast Forward
type: parsed
protocol: NECext
address: 30 FC 00 00
command: 50 AF 00 00
# 
name: Skip Forward
type: parsed
protocol: NECext
address: 30 FC 00 00
command: 13 EC 00 00
# 
name: Shuffle
type: parsed
protocol: NECext
address: 30 FC 00 00
command: 0B F4 00 00
# 
name: Repeat
type: parsed
protocol: NECext
address: 30 FC 00 00
command: 0E F1 00 00
# 
name: Up
type: parsed
protocol: NECext
address: 30 FC 00 00
command: 12 ED 00 00
# 
name: Left
type: parsed
protocol: NECext
address: 30 FC 00 00
command: 40 BF 00 00
# 
name: OK_Scan
type: parsed
protocol: NECext
address: 30 FC 00 00
command: 4C B3 00 00
# 
name: Right
type: parsed
protocol: NECext
address: 30 FC 00 00
command: 04 FB 00 00
# 
name: Down
type: parsed
protocol: NECext
address: 30 FC 00 00
command: 1E E1 00 00
# 
name: EQ
type: parsed
protocol: NECext
address: 30 FC 00 00
command: 1A E5 00 00
# 
name: MUTE
type: parsed
protocol: NECext
address: 30 FC 00 00
command: 0C F3 00 00
# 
name: Bass Up
type: parsed
protocol: NECext
address: 30 FC 00 00
command: 41 BE 00 00
# 
name: Bass Down
type: parsed
protocol: NECext
address: 30 FC 00 00
command: 42 BD 00 00
# 
name: VOL+
type: parsed
protocol: NECext
address: 30 FC 00 00
command: 0D F2 00 00
# 
name: VOL-
type: parsed
protocol: NECext
address: 30 FC 00 00
command: 17 E8 00 00
# 
name: Treble Up
type: parsed
protocol: NECext
address: 30 FC 00 00
command: 43 BC 00 00
# 
name: Treble Down
type: parsed
protocol: NECext
address: 30 FC 00 00
command: 44 BB 00 00
# 
name: 1
type: parsed
protocol: NECext
address: 30 FC 00 00
command: 09 F6 00 00
# 
name: 2 ABC
type: parsed
protocol: NECext
address: 30 FC 00 00
command: 1D E2 00 00
# 
name: 3 DEF
type: parsed
protocol: NECext
address: 30 FC 00 00
command: 1F E0 00 00
# 
name: 4 GHI
type: parsed
protocol: NECext
address: 30 FC 00 00
command: 19 E6 00 00
# 
name: 5 JKL
type: parsed
protocol: NECext
address: 30 FC 00 00
command: 1B E4 00 00
# 
name: 6 MNO
type: parsed
protocol: NECext
address: 30 FC 00 00
command: 4D B2 00 00
# 
name: 7 PQRS
type: parsed
protocol: NECext
address: 30 FC 00 00
command: 00 FF 00 00
# 
name: 8 TUV
type: parsed
protocol: NECext
address: 30 FC 00 00
command: 48 B7 00 00
# 
name: 9 WXYZ
type: parsed
protocol: NECext
address: 30 FC 00 00
command: 54 AB 00 00
# 
name: Favorites
type: parsed
protocol: NECext
address: 30 FC 00 00
command: 16 E9 00 00
# 
name: 10_0
type: parsed
protocol: NECext
address: 30 FC 00 00
command: 15 EA 00 00
# 
name: Info
type: parsed
protocol: NECext
address: 30 FC 00 00
command: 55 AA 00 00
