Filetype: IR signals file
Version: 1
#
name: X_2X
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 00 00 00 00
#
name: TITLE
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 01 00 00 00
#
name: UP
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 02 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 03 00 00 00
#
name: LEFT
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 04 00 00 00
#
name: RIGHT
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 06 00 00 00
#
name: ENTER
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 07 00 00 00
#
name: DOWN
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 08 00 00 00
#
name: ENTER
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 09 00 00 00
#
name: SLOW
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 0A 00 00 00
#
name: FORWARD
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 0C 00 00 00
#
name: PAUSE
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 0D 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 0E 00 00 00
#
name: AUDIO
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 0F 00 00 00
#
name: SCREEN
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 10 00 00 00
#
name: SUBTITLE
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 11 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 12 00 00 00
#
name: ANGLE
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 13 00 00 00
#
name: PREVIOUS
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 14 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 15 00 00 00
#
name: REWIND
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 16 00 00 00
#
name: NEXT
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 18 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 19 00 00 00
#
name: CHAPTER+
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 1A 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 1B 00 00 00
#
name: CD-DVD
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 1C 00 00 00
#
name: AGAIN
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 1D 00 00 00
#
name: CHAPTER-
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 1E 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 1F 00 00 00
