Filetype: IR signals file
Version: 1
#
name: 0
type: parsed
protocol: NECext
address: 2A 00 00 00
command: 00 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 2A 00 00 00
command: 01 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 2A 00 00 00
command: 02 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 2A 00 00 00
command: 03 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 2A 00 00 00
command: 04 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 2A 00 00 00
command: 05 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 2A 00 00 00
command: 06 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 2A 00 00 00
command: 07 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 2A 00 00 00
command: 08 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 2A 00 00 00
command: 09 00 00 00
#
name: +10
type: parsed
protocol: NECext
address: 2A 00 00 00
command: 0A 00 00 00
#
name: INTRO.
type: parsed
protocol: NECext
address: 2A 00 00 00
command: 0C 00 00 00
#
name: RANDOM
type: parsed
protocol: NECext
address: 2A 00 00 00
command: 0D 00 00 00
#
name: PLAY_>
type: parsed
protocol: NECext
address: 2A 00 00 00
command: 10 00 00 00
#
name: PAUSE/STOP
type: parsed
protocol: NECext
address: 2A 00 00 00
command: 13 00 00 00
#
name: REPEAT
type: parsed
protocol: NECext
address: 2A 00 00 00
command: 16 00 00 00
#
name: DISPLAY
type: parsed
protocol: NECext
address: 2A 00 00 00
command: 17 00 00 00
#
name: FWD_>>
type: parsed
protocol: NECext
address: 2A 00 00 00
command: 18 00 00 00
#
name: REW_<<
type: parsed
protocol: NECext
address: 2A 00 00 00
command: 19 00 00 00
#
name: SKIP_+
type: parsed
protocol: NECext
address: 2A 00 00 00
command: 1A 00 00 00
#
name: SKIP_-
type: parsed
protocol: NECext
address: 2A 00 00 00
command: 1B 00 00 00
#
name: VOLUME_UP
type: parsed
protocol: NECext
address: 2A 00 00 00
command: 1C 00 00 00
#
name: VOLUME_DOWN
type: parsed
protocol: NECext
address: 2A 00 00 00
command: 1D 00 00 00
#
name: DELETE
type: parsed
protocol: NECext
address: 2A 00 00 00
command: 55 00 00 00
