Filetype: IR signals file
Version: 1
#
name: OK
type: parsed
protocol: NECext
address: 08 00 00 00
command: 00 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 08 00 00 00
command: 01 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 08 00 00 00
command: 02 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 08 00 00 00
command: 03 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 08 00 00 00
command: 04 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 08 00 00 00
command: 05 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 08 00 00 00
command: 06 00 00 00
#
name: CHANNELUP
type: parsed
protocol: NECext
address: 08 00 00 00
command: 07 00 00 00
#
name: CURSOR_UP
type: parsed
protocol: NECext
address: 08 00 00 00
command: 08 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 08 00 00 00
command: 09 00 00 00
#
name: EPG
type: parsed
protocol: NECext
address: 08 00 00 00
command: 0B 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 08 00 00 00
command: 0C 00 00 00
#
name: SUBTITLE
type: parsed
protocol: NECext
address: 08 00 00 00
command: 0D 00 00 00
#
name: CHANNELDOWN
type: parsed
protocol: NECext
address: 08 00 00 00
command: 0E 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 08 00 00 00
command: 10 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 08 00 00 00
command: 11 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 08 00 00 00
command: 14 00 00 00
#
name: INFO
type: parsed
protocol: NECext
address: 08 00 00 00
command: 15 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 08 00 00 00
command: 18 00 00 00
#
name: CURSOR_DOWN
type: parsed
protocol: NECext
address: 08 00 00 00
command: 1B 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 08 00 00 00
command: 20 00 00 00
#
name: EXIT
type: parsed
protocol: NECext
address: 08 00 00 00
command: 21 00 00 00
#
name: RED
type: parsed
protocol: NECext
address: 08 00 00 00
command: 22 00 00 00
#
name: GREEN
type: parsed
protocol: NECext
address: 08 00 00 00
command: 23 00 00 00
#
name: YELLOW
type: parsed
protocol: NECext
address: 08 00 00 00
command: 24 00 00 00
#
name: BLUE
type: parsed
protocol: NECext
address: 08 00 00 00
command: 25 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 08 00 00 00
command: 2A 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 08 00 00 00
command: 2B 00 00 00
#
name: CURSOR_LEFT
type: parsed
protocol: NECext
address: 08 00 00 00
command: 2C 00 00 00
#
name: CURSOR_RIGHT
type: parsed
protocol: NECext
address: 08 00 00 00
command: 2D 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 08 00 00 00
command: 33 00 00 00
#
name: FAVORITES
type: parsed
protocol: NECext
address: 08 00 00 00
command: 50 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 08 00 00 00
command: 51 00 00 00
#
name: LIST
type: parsed
protocol: NECext
address: 08 00 00 00
command: 52 00 00 00
#
name: AUDIO
type: parsed
protocol: NECext
address: 08 00 00 00
command: 53 00 00 00
#
name: AB
type: parsed
protocol: NECext
address: 08 00 00 00
command: 54 00 00 00
#
name: REWIND
type: parsed
protocol: NECext
address: 08 00 00 00
command: 55 00 00 00
#
name: FASTFORWARD
type: parsed
protocol: NECext
address: 08 00 00 00
command: 56 00 00 00
#
name: CUSTOM0
type: parsed
protocol: NECext
address: 08 00 00 00
command: 60 00 00 00
#
name: RECORD
type: parsed
protocol: NECext
address: 08 00 00 00
command: 61 00 00 00
