Filetype: IR signals file
Version: 1
#
name: CLEAR
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 06 00 00 00
#
name: DONE
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 06 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 08 00 00 00
#
name: RESET
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 12 00 00 00
#
name: PREV_CHANNEL
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 27 00 00 00
#
name: PREV_CH
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 27 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 2A 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 2A 00 00 00
#
name: CHANNEL_-
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 2C 00 00 00
#
name: CHANNEL_-
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 2C 00 00 00
#
name: CURSOR_V
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 2C 00 00 00
#
name: CHANNEL_+
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 2D 00 00 00
#
name: CHANNEL_+
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 2D 00 00 00
#
name: CURSOR_^
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 2D 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 2E 00 00 00
#
name: CURSOR_-
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 2E 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 2F 00 00 00
#
name: CURSOR_+
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 2F 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 2F 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 30 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 30 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 31 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 31 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 32 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 32 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 33 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 33 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 34 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 34 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 35 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 35 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 36 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 36 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 37 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 37 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 38 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 38 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 39 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 39 00 00 00
#
name: POWER_ON
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 3A 00 00 00
#
name: POWER_OFF
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 3B 00 00 00
#
name: DISPLAY
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 3C 00 00 00
#
name: DISPLAY
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 3C 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 3F 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 3F 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 52 00 00 00
#
name: SKIP
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 53 00 00 00
#
name: SKIP:30
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 53 00 00 00
#
name: INPUT_SOURCE
type: parsed
protocol: NECext
address: 0F 00 00 00
command: A3 00 00 00
#
name: INPUT
type: parsed
protocol: NECext
address: 0F 00 00 00
command: A3 00 00 00
