Filetype: IR signals file
Version: 1
#
name: surround+
type: parsed
protocol: NECext
address: 08 00 00 00
command: 00 00 00 00
#
name: SUBTITLE
type: parsed
protocol: NECext
address: 08 00 00 00
command: 01 00 00 00
#
name: center+
type: parsed
protocol: NECext
address: 08 00 00 00
command: 02 00 00 00
#
name: SUBTITLE
type: parsed
protocol: NECext
address: 08 00 00 00
command: 03 00 00 00
#
name: surround-
type: parsed
protocol: NECext
address: 08 00 00 00
command: 04 00 00 00
#
name: test
type: parsed
protocol: NECext
address: 08 00 00 00
command: 05 00 00 00
#
name: center-
type: parsed
protocol: NECext
address: 08 00 00 00
command: 06 00 00 00
#
name: direct
type: parsed
protocol: NECext
address: 08 00 00 00
command: 0A 00 00 00
#
name: optical
type: parsed
protocol: NECext
address: 08 00 00 00
command: 0B 00 00 00
#
name: coax
type: parsed
protocol: NECext
address: 08 00 00 00
command: 0C 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 08 00 00 00
command: 0E 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 08 00 00 00
command: 10 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 08 00 00 00
command: 16 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 08 00 00 00
command: 1A 00 00 00
#
name: effect
type: parsed
protocol: NECext
address: 08 00 00 00
command: 1D 00 00 00
#
name: SETUP
type: parsed
protocol: NECext
address: 08 00 00 00
command: 1F 00 00 00
