Filetype: IR signals file
Version: 1
#
name: POWER
type: parsed
protocol: NECext
address: 7B 00 00 00
command: 00 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 7B 00 00 00
command: 01 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 7B 00 00 00
command: 02 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 7B 00 00 00
command: 03 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 7B 00 00 00
command: 04 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 7B 00 00 00
command: 05 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 7B 00 00 00
command: 06 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 7B 00 00 00
command: 07 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 7B 00 00 00
command: 08 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 7B 00 00 00
command: 09 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 7B 00 00 00
command: 0A 00 00 00
#
name: YELLOW
type: parsed
protocol: NECext
address: 7B 00 00 00
command: 13 00 00 00
#
name: RIGHT
type: parsed
protocol: NECext
address: 7B 00 00 00
command: 18 00 00 00
#
name: LEFT
type: parsed
protocol: NECext
address: 7B 00 00 00
command: 19 00 00 00
#
name: OK
type: parsed
protocol: NECext
address: 7B 00 00 00
command: 1B 00 00 00
#
name: UP
type: parsed
protocol: NECext
address: 7B 00 00 00
command: 40 00 00 00
#
name: DOWN
type: parsed
protocol: NECext
address: 7B 00 00 00
command: 41 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 7B 00 00 00
command: 43 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 7B 00 00 00
command: 4A 00 00 00
#
name: BLUE
type: parsed
protocol: NECext
address: 7B 00 00 00
command: 4B 00 00 00
#
name: RED
type: parsed
protocol: NECext
address: 7B 00 00 00
command: 4E 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 7B 00 00 00
command: 4F 00 00 00
#
name: BACK
type: parsed
protocol: NECext
address: 7B 00 00 00
command: 90 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 7B 00 00 00
command: C4 00 00 00
#
name: GREEN
type: parsed
protocol: NECext
address: 7B 00 00 00
command: DC 00 00 00
