Filetype: IR signals file
Version: 1
# 
name: POWER
type: parsed
protocol: NECext
address: 08 16 00 00
command: 87 78 00 00
# 
name: Src
type: parsed
protocol: NECext
address: 08 16 00 00
command: DC 23 00 00
# 
name: Menu
type: parsed
protocol: NECext
address: 08 16 00 00
command: 8A 75 00 00
# 
name: Back
type: parsed
protocol: NECext
address: 08 16 00 00
command: 8B 74 00 00
# 
name: Up
type: parsed
protocol: NECext
address: 08 16 00 00
command: 84 7B 00 00
# 
name: Dwn
type: parsed
protocol: NECext
address: 08 16 00 00
command: 8D 72 00 00
# 
name: Left
type: parsed
protocol: NECext
address: 08 16 00 00
command: BB 44 00 00
# 
name: Right
type: parsed
protocol: NECext
address: 08 16 00 00
command: 8E 71 00 00
# 
name: Ok
type: parsed
protocol: NECext
address: 08 16 00 00
command: B2 4D 00 00
# 
name: Vup
type: parsed
protocol: NECext
address: 08 16 00 00
command: 89 76 00 00
# 
name: Vdwn
type: parsed
protocol: NECext
address: 08 16 00 00
command: B5 4A 00 00
# 
name: MUTE
type: parsed
protocol: NECext
address: 08 16 00 00
command: C8 37 00 00
