Filetype: IR signals file
Version: 1
#
name: VIEW_TV
type: parsed
protocol: NECext
address: 08 00 00 00
command: 16 00 00 00
#
name: VCR
type: parsed
protocol: NECext
address: 08 00 00 00
command: 2B 00 00 00
