Filetype: IR signals file
Version: 1
#
name: STOP
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 00 00 00 00
#
name: EJECTCD
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 01 00 00 00
#
name: searCH-
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 02 00 00 00
#
name: search_up
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 03 00 00 00
#
name: PAUSE
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 06 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 0A 00 00 00
#
name: num_1
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 10 00 00 00
#
name: num_2
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 11 00 00 00
#
name: num_3
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 11 00 00 00
#
name: num_4
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 13 00 00 00
#
name: num_5
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 14 00 00 00
#
name: num_6
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 15 00 00 00
#
name: num_7
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 16 00 00 00
#
name: num_8
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 17 00 00 00
#
name: num_9
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 18 00 00 00
#
name: num_0
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 19 00 00 00
#
name: level_up
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 20 00 00 00
#
name: level_down
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 21 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 3D 00 00 00
#
name: AGAIN
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 47 00 00 00
#
name: a-b_repeat
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 48 00 00 00
#
name: skip_down
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 49 00 00 00
#
name: skip_up
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 4A 00 00 00
#
name: random
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 4D 00 00 00
#
name: time_mode
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 55 00 00 00
#
name: CLEAR
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 80 00 00 00
#
name: AGAIN
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 81 00 00 00
#
name: two_digits
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 84 00 00 00
#
name: program
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 8A 00 00 00
#
name: auto_cue
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 8B 00 00 00
#
name: peak_search
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 8F 00 00 00
#
name: time_fade
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 94 00 00 00
#
name: tape_length
type: parsed
protocol: NECext
address: A0 0A 00 00
command: AB 00 00 00
#
name: side_a-b
type: parsed
protocol: NECext
address: A0 0A 00 00
command: AC 00 00 00
