Filetype: IR signals file
Version: 1
#
name: VOLUME_UP
type: parsed
protocol: NECext
address: 77 00 00 00
command: 22 00 00 00
#
name: VOLUME_DOWN
type: parsed
protocol: NECext
address: 77 00 00 00
command: 2A 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 77 00 00 00
command: 32 00 00 00
#
name: VCR_A
type: parsed
protocol: NECext
address: 77 00 00 00
command: 44 00 00 00
