Filetype: IR signals file
Version: 1
#
name: 0
type: parsed
protocol: NECext
address: 00 0C 00 00
command: 00 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 00 0C 00 00
command: 01 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 00 0C 00 00
command: 02 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 00 0C 00 00
command: 03 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 00 0C 00 00
command: 04 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 00 0C 00 00
command: 05 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 00 0C 00 00
command: 06 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 00 0C 00 00
command: 07 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 00 0C 00 00
command: 08 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 00 0C 00 00
command: 09 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 00 0C 00 00
command: 0C 00 00 00
#
name: CHANNELUP
type: parsed
protocol: NECext
address: 00 0C 00 00
command: 20 00 00 00
#
name: CHANNELDOWN
type: parsed
protocol: NECext
address: 00 0C 00 00
command: 21 00 00 00
#
name: PAUSE
type: parsed
protocol: NECext
address: 00 0C 00 00
command: 24 00 00 00
#
name: FASTFORWARD
type: parsed
protocol: NECext
address: 00 0C 00 00
command: 28 00 00 00
#
name: TEXT
type: parsed
protocol: NECext
address: 00 0C 00 00
command: 3C 00 00 00
#
name: FREV
type: parsed
protocol: NECext
address: 00 0C 00 00
command: 3D 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 00 0C 00 00
command: 3E 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 00 0C 00 00
command: 3F 00 00 00
#
name: RECORD
type: parsed
protocol: NECext
address: 00 0C 00 00
command: 40 00 00 00
#
name: UP
type: parsed
protocol: NECext
address: 00 0C 00 00
command: 58 00 00 00
#
name: DOWN
type: parsed
protocol: NECext
address: 00 0C 00 00
command: 59 00 00 00
#
name: LEFT
type: parsed
protocol: NECext
address: 00 0C 00 00
command: 5A 00 00 00
#
name: RIGHT
type: parsed
protocol: NECext
address: 00 0C 00 00
command: 5B 00 00 00
#
name: SELECT
type: parsed
protocol: NECext
address: 00 0C 00 00
command: 5C 00 00 00
#
name: RED
type: parsed
protocol: NECext
address: 00 0C 00 00
command: 6D 00 00 00
#
name: GREEN
type: parsed
protocol: NECext
address: 00 0C 00 00
command: 6E 00 00 00
#
name: YELLOW
type: parsed
protocol: NECext
address: 00 0C 00 00
command: 6F 00 00 00
#
name: BLUE
type: parsed
protocol: NECext
address: 00 0C 00 00
command: 70 00 00 00
#
name: BOX_OFFICE
type: parsed
protocol: NECext
address: 00 0C 00 00
command: 7D 00 00 00
#
name: SERVICES
type: parsed
protocol: NECext
address: 00 0C 00 00
command: 7E 00 00 00
#
name: SKY
type: parsed
protocol: NECext
address: 00 0C 00 00
command: 80 00 00 00
#
name: HELP
type: parsed
protocol: NECext
address: 00 0C 00 00
command: 81 00 00 00
#
name: BACK_UP
type: parsed
protocol: NECext
address: 00 0C 00 00
command: 83 00 00 00
#
name: TV
type: parsed
protocol: NECext
address: 00 0C 00 00
command: 84 00 00 00
#
name: INFO
type: parsed
protocol: NECext
address: 00 0C 00 00
command: CB 00 00 00
#
name: TV_GUIDE
type: parsed
protocol: NECext
address: 00 0C 00 00
command: CC 00 00 00
#
name: INTERACTIVE
type: parsed
protocol: NECext
address: 00 0C 00 00
command: F5 00 00 00
