Filetype: IR signals file
Version: 1
# 
name: POWER
type: parsed
protocol: NEC
address: 80 00 00 00
command: 12 00 00 00
# 
name: 1
type: parsed
protocol: NEC
address: 80 00 00 00
command: 01 00 00 00
# 
name: 2
type: parsed
protocol: NEC
address: 80 00 00 00
command: 02 00 00 00
# 
name: 3
type: parsed
protocol: NEC
address: 80 00 00 00
command: 03 00 00 00
# 
name: 4
type: parsed
protocol: NEC
address: 80 00 00 00
command: 04 00 00 00
# 
name: 5
type: parsed
protocol: NEC
address: 80 00 00 00
command: 05 00 00 00
# 
name: 6
type: parsed
protocol: NEC
address: 80 00 00 00
command: 06 00 00 00
# 
name: 7
type: parsed
protocol: NEC
address: 80 00 00 00
command: 07 00 00 00
# 
name: 8
type: parsed
protocol: NEC
address: 80 00 00 00
command: 08 00 00 00
# 
name: 9
type: parsed
protocol: NEC
address: 80 00 00 00
command: 09 00 00 00
# 
name: ok
type: parsed
protocol: NEC
address: 80 00 00 00
command: 0A 00 00 00
# 
name: source
type: parsed
protocol: NEC
address: 80 00 00 00
command: 14 00 00 00
# 
name: o
type: parsed
protocol: NEC
address: 80 00 00 00
command: 00 00 00 00
# 
name: up
type: parsed
protocol: NEC
address: 80 00 00 00
command: 19 00 00 00
# 
name: down
type: parsed
protocol: NEC
address: 80 00 00 00
command: 1D 00 00 00
# 
name: left
type: parsed
protocol: NEC
address: 80 00 00 00
command: 46 00 00 00
# 
name: right
type: parsed
protocol: NEC
address: 80 00 00 00
command: 47 00 00 00
# 
name: back
type: parsed
protocol: NEC
address: 80 00 00 00
command: 44 00 00 00
# 
name: menu
type: parsed
protocol: NEC
address: 80 00 00 00
command: 5B 00 00 00
# 
name: VOL+
type: parsed
protocol: NEC
address: 80 00 00 00
command: 1A 00 00 00
# 
name: VOL-
type: parsed
protocol: NEC
address: 80 00 00 00
command: 1E 00 00 00
# 
name: MUTE
type: parsed
protocol: NEC
address: 80 00 00 00
command: 10 00 00 00
