Filetype: IR signals file
Version: 1
#
# MPMAN XV-D505HDMI
# Autogenerated from ircodes/MPMAN/XV-D505HDMI.xml
#
name: POWER
type: parsed
protocol: NECext
address: FF 00 00 00
command: CF 30 00 00
#
name: Unknown
type: parsed
protocol: NECext
address: FF 00 00 00
command: F5 0A 00 00
#
name: DVD/TV
type: parsed
protocol: NECext
address: FF 00 00 00
command: 4F B0 00 00
#
name: 1
type: parsed
protocol: NECext
address: FF 00 00 00
command: FF 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: FF 00 00 00
command: 7F 80 00 00
#
name: 3
type: parsed
protocol: NECext
address: FF 00 00 00
command: BF 40 00 00
#
name: 4
type: parsed
protocol: NECext
address: FF 00 00 00
command: 3F C0 00 00
#
name: 5
type: parsed
protocol: NECext
address: FF 00 00 00
command: DF 20 00 00
#
name: 6
type: parsed
protocol: NECext
address: FF 00 00 00
command: 5F A0 00 00
#
name: 7
type: parsed
protocol: NECext
address: FF 00 00 00
command: 9F 60 00 00
#
name: 8
type: parsed
protocol: NECext
address: FF 00 00 00
command: 1F E0 00 00
#
name: 9
type: parsed
protocol: NECext
address: FF 00 00 00
command: EF 10 00 00
#
name: +10
type: parsed
protocol: NECext
address: FF 00 00 00
command: AF 50 00 00
#
name: 0
type: parsed
protocol: NECext
address: FF 00 00 00
command: 6F 90 00 00
#
name: C/CH
type: parsed
protocol: NECext
address: FF 00 00 00
command: 07 F8 00 00
#
name: Top Menu
type: parsed
protocol: NECext
address: FF 00 00 00
command: B5 4A 00 00
#
name: Unknown
type: parsed
protocol: NECext
address: FF 00 00 00
command: F7 08 00 00
#
name: Title
type: parsed
protocol: NECext
address: FF 00 00 00
command: 97 68 00 00
#
name: Unknown
type: parsed
protocol: NECext
address: FF 00 00 00
command: B7 48 00 00
#
name: OK
type: parsed
protocol: NECext
address: FF 00 00 00
command: 8F 70 00 00
#
name: Unknown
type: parsed
protocol: NECext
address: FF 00 00 00
command: 37 C8 00 00
#
name: Menu
type: parsed
protocol: NECext
address: FF 00 00 00
command: 57 A8 00 00
#
name: Unknown
type: parsed
protocol: NECext
address: FF 00 00 00
command: 77 88 00 00
#
name: Repeat/1/All
type: parsed
protocol: NECext
address: FF 00 00 00
command: 75 8A 00 00
#
name: Return
type: parsed
protocol: NECext
address: FF 00 00 00
command: A7 58 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: FF 00 00 00
command: 0D F2 00 00
#
name: Display
type: parsed
protocol: NECext
address: FF 00 00 00
command: 87 78 00 00
#
name: PREV
type: parsed
protocol: NECext
address: FF 00 00 00
command: BD 42 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: FF 00 00 00
command: 35 CA 00 00
#
name: Rep/A-B
type: parsed
protocol: NECext
address: FF 00 00 00
command: 4D B2 00 00
#
name: NEXT
type: parsed
protocol: NECext
address: FF 00 00 00
command: 3D C2 00 00
#
name: Auto/Track
type: parsed
protocol: NECext
address: FF 00 00 00
command: 2F D0 00 00
#
name: SUBTITLE
type: parsed
protocol: NECext
address: FF 00 00 00
command: 17 E8 00 00
#
name: Zoom
type: parsed
protocol: NECext
address: FF 00 00 00
command: 27 D8 00 00
#
name: PROG
type: parsed
protocol: NECext
address: FF 00 00 00
command: 47 B8 00 00
#
name: Slow -
type: parsed
protocol: NECext
address: FF 00 00 00
command: 2D D2 00 00
#
name: Slow +
type: parsed
protocol: NECext
address: FF 00 00 00
command: 8D 72 00 00
#
name: STOP
type: parsed
protocol: NECext
address: FF 00 00 00
command: 5D A2 00 00
#
name: PAUSE
type: parsed
protocol: NECext
address: FF 00 00 00
command: CD 32 00 00
#
name: REC
type: parsed
protocol: NECext
address: FF 00 00 00
command: E7 18 00 00
#
name: REW
type: parsed
protocol: NECext
address: FF 00 00 00
command: FD 02 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: FF 00 00 00
command: DD 22 00 00
#
name: FWD
type: parsed
protocol: NECext
address: FF 00 00 00
command: 7D 82 00 00
#
name: EJECT
type: parsed
protocol: NECext
address: FF 00 00 00
command: 4F B0 00 00
#
name: 3D
type: parsed
protocol: NECext
address: FF 00 00 00
command: 6D 92 00 00
#
name: Audio
type: parsed
protocol: NECext
address: FF 00 00 00
command: ED 12 00 00
#
name: Video
type: parsed
protocol: NECext
address: FF 00 00 00
command: 07 F8 00 00
#
name: Search
type: parsed
protocol: NECext
address: FF 00 00 00
command: 2F D0 00 00
#
name: Pbc
type: parsed
protocol: NECext
address: FF 00 00 00
command: 67 98 00 00
#
name: R/L
type: parsed
protocol: NECext
address: FF 00 00 00
command: CD 32 00 00
#
name: Echo+
type: parsed
protocol: NECext
address: FF 00 00 00
command: 8D 72 00 00
#
name: Setup
type: parsed
protocol: NECext
address: FF 00 00 00
command: D7 28 00 00
#
name: Echo-
type: parsed
protocol: NECext
address: FF 00 00 00
command: B5 4A 00 00
#
name: Np
type: parsed
protocol: NECext
address: FF 00 00 00
command: C7 38 00 00
#
name: Resume
type: parsed
protocol: NECext
address: FF 00 00 00
command: 6D 92 00 00
#
name: Karaoke/Step
type: parsed
protocol: NECext
address: FF 00 00 00
command: AD 52 00 00
#
name: Angle
type: parsed
protocol: NECext
address: FF 00 00 00
command: E7 18 00 00
#
name: Shuffle
type: parsed
protocol: NECext
address: FF 00 00 00
command: B5 4A 00 00
