Filetype: IR signals file
Version: 1
#
name: 0
type: parsed
protocol: NECext
address: 05 00 00 00
command: 00 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 05 00 00 00
command: 01 00 00 00
#
name: QP_START_+_1
type: parsed
protocol: NECext
address: 05 00 00 00
command: 01 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 05 00 00 00
command: 02 00 00 00
#
name: QP_STOP_+_2
type: parsed
protocol: NECext
address: 05 00 00 00
command: 02 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 05 00 00 00
command: 03 00 00 00
#
name: QP_DATE_+_3
type: parsed
protocol: NECext
address: 05 00 00 00
command: 03 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 05 00 00 00
command: 04 00 00 00
#
name: QP_START_-_4
type: parsed
protocol: NECext
address: 05 00 00 00
command: 04 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 05 00 00 00
command: 05 00 00 00
#
name: QP_STOP_-_5
type: parsed
protocol: NECext
address: 05 00 00 00
command: 05 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 05 00 00 00
command: 06 00 00 00
#
name: QP_DATE_-_6
type: parsed
protocol: NECext
address: 05 00 00 00
command: 06 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 05 00 00 00
command: 07 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 05 00 00 00
command: 08 00 00 00
#
name: QP_DAILY_8
type: parsed
protocol: NECext
address: 05 00 00 00
command: 08 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 05 00 00 00
command: 09 00 00 00
#
name: QP_WEEKLY_9
type: parsed
protocol: NECext
address: 05 00 00 00
command: 09 00 00 00
#
name: 100
type: parsed
protocol: NECext
address: 05 00 00 00
command: 0A 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 05 00 00 00
command: 0C 00 00 00
#
name: VCR_POWER
type: parsed
protocol: NECext
address: 05 00 00 00
command: 0C 00 00 00
#
name: TURBO_TIMER
type: parsed
protocol: NECext
address: 05 00 00 00
command: 1C 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 05 00 00 00
command: 1D 00 00 00
#
name: CH_+
type: parsed
protocol: NECext
address: 05 00 00 00
command: 20 00 00 00
#
name: VCR_CH_+
type: parsed
protocol: NECext
address: 05 00 00 00
command: 20 00 00 00
#
name: CH_-
type: parsed
protocol: NECext
address: 05 00 00 00
command: 21 00 00 00
#
name: VCR_CH_-
type: parsed
protocol: NECext
address: 05 00 00 00
command: 21 00 00 00
#
name: AUDIO/MUTE
type: parsed
protocol: NECext
address: 05 00 00 00
command: 23 00 00 00
#
name: AUDIO
type: parsed
protocol: NECext
address: 05 00 00 00
command: 23 00 00 00
#
name: SLOW_MOTION_-
type: parsed
protocol: NECext
address: 05 00 00 00
command: 25 00 00 00
#
name: PLAY_SPEED_DOWN
type: parsed
protocol: NECext
address: 05 00 00 00
command: 25 00 00 00
#
name: SLOW_MOTION_+
type: parsed
protocol: NECext
address: 05 00 00 00
command: 26 00 00 00
#
name: PLAY_SPEED_UP
type: parsed
protocol: NECext
address: 05 00 00 00
command: 26 00 00 00
#
name: OTR
type: parsed
protocol: NECext
address: 05 00 00 00
command: 27 00 00 00
#
name: VAR_PLAY
type: parsed
protocol: NECext
address: 05 00 00 00
command: 28 00 00 00
#
name: PAUSE/SLOW
type: parsed
protocol: NECext
address: 05 00 00 00
command: 29 00 00 00
#
name: PAUSE/STILL
type: parsed
protocol: NECext
address: 05 00 00 00
command: 29 00 00 00
#
name: EJECT
type: parsed
protocol: NECext
address: 05 00 00 00
command: 2D 00 00 00
#
name: CLEAR
type: parsed
protocol: NECext
address: 05 00 00 00
command: 31 00 00 00
#
name: REWIND_<<
type: parsed
protocol: NECext
address: 05 00 00 00
command: 32 00 00 00
#
name: FAST_FORWARD_>>
type: parsed
protocol: NECext
address: 05 00 00 00
command: 34 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 05 00 00 00
command: 35 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 05 00 00 00
command: 36 00 00 00
#
name: RECORD
type: parsed
protocol: NECext
address: 05 00 00 00
command: 37 00 00 00
#
name: QP_SPEED
type: parsed
protocol: NECext
address: 05 00 00 00
command: 3A 00 00 00
#
name: SP/SLP
type: parsed
protocol: NECext
address: 05 00 00 00
command: 3A 00 00 00
#
name: MEMO
type: parsed
protocol: NECext
address: 05 00 00 00
command: 3B 00 00 00
#
name: CLK/CNT
type: parsed
protocol: NECext
address: 05 00 00 00
command: 3C 00 00 00
#
name: VCR/TV
type: parsed
protocol: NECext
address: 05 00 00 00
command: 3E 00 00 00
#
name: TIMER
type: parsed
protocol: NECext
address: 05 00 00 00
command: 45 00 00 00
#
name: VCR_PLUS:_DAILY
type: parsed
protocol: NECext
address: 05 00 00 00
command: 45 00 00 00
#
name: SMART_PICTURE
type: parsed
protocol: NECext
address: 05 00 00 00
command: 46 00 00 00
#
name: PICT_CTRL
type: parsed
protocol: NECext
address: 05 00 00 00
command: 46 00 00 00
#
name: TRACKING_+
type: parsed
protocol: NECext
address: 05 00 00 00
command: 4D 00 00 00
#
name: TRACKING_-
type: parsed
protocol: NECext
address: 05 00 00 00
command: 4E 00 00 00
#
name: TAPE_MANAGER
type: parsed
protocol: NECext
address: 05 00 00 00
command: 4F 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 05 00 00 00
command: 52 00 00 00
#
name: OK/STATUS
type: parsed
protocol: NECext
address: 05 00 00 00
command: 57 00 00 00
#
name: SKIP/SEARCH
type: parsed
protocol: NECext
address: 05 00 00 00
command: 6A 00 00 00
#
name: SKIP
type: parsed
protocol: NECext
address: 05 00 00 00
command: 6A 00 00 00
#
name: VISS_FWD
type: parsed
protocol: NECext
address: 05 00 00 00
command: 70 00 00 00
#
name: VISS_REV
type: parsed
protocol: NECext
address: 05 00 00 00
command: 71 00 00 00
