Filetype: IR signals file
Version: 1
#
name: STOP
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 00 00 00 00
#
name: OPEN
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 01 00 00 00
#
name: REWIND
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 02 00 00 00
#
name: FASTFORWARD
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 03 00 00 00
#
name: PAUSE
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 06 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 0A 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 10 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 11 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 12 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 13 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 14 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 15 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 16 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 17 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 18 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 19 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 20 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 21 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 3D 00 00 00
#
name: AGAIN
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 47 00 00 00
#
name: A\*B_Repeat
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 48 00 00 00
#
name: PrevTrack
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 49 00 00 00
#
name: NEXT
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 4A 00 00 00
#
name: Random
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 4D 00 00 00
#
name: Time_Mode
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 55 00 00 00
#
name: CLEAR
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 80 00 00 00
#
name: AGAIN
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 81 00 00 00
#
name: >10
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 84 00 00 00
#
name: Program
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 8A 00 00 00
#
name: Auto_Cue
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 8B 00 00 00
#
name: Peak_Search
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 8F 00 00 00
#
name: Time_Fade
type: parsed
protocol: NECext
address: A0 0A 00 00
command: 94 00 00 00
#
name: Tape_Length
type: parsed
protocol: NECext
address: A0 0A 00 00
command: AB 00 00 00
#
name: Side_A/B
type: parsed
protocol: NECext
address: A0 0A 00 00
command: AC 00 00 00
