Filetype: IR signals file
Version: 1
#
name: MUTE
type: parsed
protocol: NECext
address: 01 00 00 00
command: 06 00 00 00
#
name: CHANNELUP
type: parsed
protocol: NECext
address: 01 00 00 00
command: 07 00 00 00
#
name: CHANNELDOWN
type: parsed
protocol: NECext
address: 01 00 00 00
command: 08 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 01 00 00 00
command: 2E 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 01 00 00 00
command: 2F 00 00 00
