Filetype: IR signals file
Version: 1
# 
name: POWER
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 02 00 00 00
# 
name: VOL+
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 07 00 00 00
# 
name: VOL-
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 0B 00 00 00
# 
name: MUTE
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 0F 00 00 00
# 
name: CH+
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 12 00 00 00
# 
name: CH-
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 10 00 00 00
# 
name: RETURN
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 58 00 00 00
# 
name: EXIT
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 2D 00 00 00
# 
name: OK
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 68 00 00 00
# 
name: UP
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 60 00 00 00
# 
name: DOWN
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 61 00 00 00
# 
name: LEFT
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 65 00 00 00
# 
name: RIGHT
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 62 00 00 00
# 
name: SOURCE
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 01 00 00 00
# 
name: MENU
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 1A 00 00 00
# 
name: GUIDE
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 4F 00 00 00
# 
name: TOOLS
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 4B 00 00 00
