Filetype: IR signals file
Version: 1
#
name: 0
type: parsed
protocol: NECext
address: 05 00 00 00
command: 00 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 05 00 00 00
command: 01 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 05 00 00 00
command: 02 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 05 00 00 00
command: 03 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 05 00 00 00
command: 04 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 05 00 00 00
command: 05 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 05 00 00 00
command: 06 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 05 00 00 00
command: 07 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 05 00 00 00
command: 08 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 05 00 00 00
command: 09 00 00 00
#
name: switch_prgs
type: parsed
protocol: NECext
address: 05 00 00 00
command: 0A 00 00 00
#
name: SLEEP
type: parsed
protocol: NECext
address: 05 00 00 00
command: 0C 00 00 00
#
name: calibrate
type: parsed
protocol: NECext
address: 05 00 00 00
command: 0E 00 00 00
#
name: prog
type: parsed
protocol: NECext
address: 05 00 00 00
command: 1D 00 00 00
#
name: UP
type: parsed
protocol: NECext
address: 05 00 00 00
command: 20 00 00 00
#
name: DOWN
type: parsed
protocol: NECext
address: 05 00 00 00
command: 21 00 00 00
#
name: otr-rec
type: parsed
protocol: NECext
address: 05 00 00 00
command: 24 00 00 00
#
name: PAUSE
type: parsed
protocol: NECext
address: 05 00 00 00
command: 29 00 00 00
#
name: fast
type: parsed
protocol: NECext
address: 05 00 00 00
command: 2A 00 00 00
#
name: pic_rew
type: parsed
protocol: NECext
address: 05 00 00 00
command: 2C 00 00 00
#
name: pic_ff
type: parsed
protocol: NECext
address: 05 00 00 00
command: 2E 00 00 00
#
name: REWIND
type: parsed
protocol: NECext
address: 05 00 00 00
command: 2F 00 00 00
#
name: reset
type: parsed
protocol: NECext
address: 05 00 00 00
command: 31 00 00 00
#
name: REWIND
type: parsed
protocol: NECext
address: 05 00 00 00
command: 32 00 00 00
#
name: FASTFORWARD
type: parsed
protocol: NECext
address: 05 00 00 00
command: 34 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 05 00 00 00
command: 35 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 05 00 00 00
command: 36 00 00 00
#
name: RECORD
type: parsed
protocol: NECext
address: 05 00 00 00
command: 37 00 00 00
