Filetype: IR signals file
Version: 1
#
# For Adstra WA215 Wall & Ceiling Speaker Set
# 
name: POWER
type: parsed
protocol: NEC
address: 00 00 00 00
command: 45 00 00 00
# 
name: VOL+
type: parsed
protocol: NEC
address: 00 00 00 00
command: 19 00 00 00
# 
name: VOL-
type: parsed
protocol: NEC
address: 00 00 00 00
command: 16 00 00 00
# 
name: Pause
type: parsed
protocol: NEC
address: 00 00 00 00
command: 09 00 00 00
# 
name: MUTE
type: parsed
protocol: NEC
address: 00 00 00 00
command: 44 00 00 00
# 
name: Music
type: parsed
protocol: NEC
address: 00 00 00 00
command: 46 00 00 00
# 
name: Bluetooth
type: parsed
protocol: NEC
address: 00 00 00 00
command: 47 00 00 00
# 
name: Next
type: parsed
protocol: NEC
address: 00 00 00 00
command: 15 00 00 00
# 
name: Previous
type: parsed
protocol: NEC
address: 00 00 00 00
command: 07 00 00 00
# 
name: FM
type: parsed
protocol: NEC
address: 00 00 00 00
command: 40 00 00 00
# 
name: VF
type: parsed
protocol: NEC
address: 00 00 00 00
command: 43 00 00 00
# 
name: Aux_in
type: parsed
protocol: NEC
address: 00 00 00 00
command: 41 00 00 00
# 
name: Back
type: parsed
protocol: NEC
address: 00 00 00 00
command: 49 00 00 00
# 
name: AV
type: parsed
protocol: NEC
address: 00 00 00 00
command: 42 00 00 00
