Filetype: IR signals file
Version: 1
#
name: 0
type: parsed
protocol: NECext
address: 40 00 00 00
command: 00 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 40 00 00 00
command: 01 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 40 00 00 00
command: 02 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 40 00 00 00
command: 03 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 40 00 00 00
command: 04 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 40 00 00 00
command: 05 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 40 00 00 00
command: 06 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 40 00 00 00
command: 07 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 40 00 00 00
command: 08 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 40 00 00 00
command: 09 00 00 00
#
name: VIDEO
type: parsed
protocol: NECext
address: 40 00 00 00
command: 0D 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 40 00 00 00
command: 10 00 00 00
#
name: picture_preset
type: parsed
protocol: NECext
address: 40 00 00 00
command: 11 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 40 00 00 00
command: 12 00 00 00
#
name: audio_stereo_2channel
type: parsed
protocol: NECext
address: 40 00 00 00
command: 13 00 00 00
#
name: CYCLEWINDOWS
type: parsed
protocol: NECext
address: 40 00 00 00
command: 14 00 00 00
#
name: TIME
type: parsed
protocol: NECext
address: 40 00 00 00
command: 15 00 00 00
#
name: INFO
type: parsed
protocol: NECext
address: 40 00 00 00
command: 16 00 00 00
#
name: VIDEO
type: parsed
protocol: NECext
address: 40 00 00 00
command: 17 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 40 00 00 00
command: 1A 00 00 00
#
name: p_up
type: parsed
protocol: NECext
address: 40 00 00 00
command: 1B 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 40 00 00 00
command: 1E 00 00 00
#
name: p_down
type: parsed
protocol: NECext
address: 40 00 00 00
command: 1F 00 00 00
#
name: OK
type: parsed
protocol: NECext
address: 40 00 00 00
command: 21 00 00 00
#
name: stillpicture
type: parsed
protocol: NECext
address: 40 00 00 00
command: 22 00 00 00
#
name: VIDEO
type: parsed
protocol: NECext
address: 40 00 00 00
command: 2B 00 00 00
#
name: VIDEO
type: parsed
protocol: NECext
address: 40 00 00 00
command: 2C 00 00 00
#
name: EXIT
type: parsed
protocol: NECext
address: 40 00 00 00
command: 43 00 00 00
#
name: RED
type: parsed
protocol: NECext
address: 40 00 00 00
command: 48 00 00 00
#
name: GREEN
type: parsed
protocol: NECext
address: 40 00 00 00
command: 49 00 00 00
#
name: YELLOW
type: parsed
protocol: NECext
address: 40 00 00 00
command: 4A 00 00 00
#
name: BLUE
type: parsed
protocol: NECext
address: 40 00 00 00
command: 4B 00 00 00
#
name: BACK
type: parsed
protocol: NECext
address: 40 00 00 00
command: 52 00 00 00
#
name: VIDEO
type: parsed
protocol: NECext
address: 40 00 00 00
command: 53 00 00 00
#
name: VIDEO
type: parsed
protocol: NECext
address: 40 00 00 00
command: 54 00 00 00
#
name: widescreen
type: parsed
protocol: NECext
address: 40 00 00 00
command: 59 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 40 00 00 00
command: 5B 00 00 00
