Filetype: IR signals file
Version: 1
# 
name: Power
type: parsed
protocol: NECext
address: 02 A0 00 00
command: 80 7F 00 00
# 
name: Plus
type: parsed
protocol: NECext
address: 02 A0 00 00
command: AA 55 00 00
# 
name: Minus
type: parsed
protocol: NECext
address: 02 A0 00 00
command: 6A 95 00 00
# 
name: Mute
type: parsed
protocol: NECext
address: 02 A0 00 00
command: EA 15 00 00
# 
name: Input
type: parsed
protocol: NECext
address: 02 A0 00 00
command: 08 F7 00 00
# 
name: Effect
type: parsed
protocol: NECext
address: 02 A0 00 00
command: 0E F1 00 00