Filetype: IR signals file
Version: 1
#
name: VOL+
type: parsed
protocol: NECext
address: 05 01 00 00
command: 02 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 05 01 00 00
command: 0A 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 05 01 00 00
command: 0B 00 00 00
