Filetype: IR signals file
Version: 1
#
name: 0
type: parsed
protocol: NECext
address: 05 00 00 00
command: 00 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 05 00 00 00
command: 01 00 00 00
#
name: START+
type: parsed
protocol: NECext
address: 05 00 00 00
command: 01 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 05 00 00 00
command: 02 00 00 00
#
name: STOP_+
type: parsed
protocol: NECext
address: 05 00 00 00
command: 02 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 05 00 00 00
command: 03 00 00 00
#
name: DATE_+
type: parsed
protocol: NECext
address: 05 00 00 00
command: 03 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 05 00 00 00
command: 04 00 00 00
#
name: START-
type: parsed
protocol: NECext
address: 05 00 00 00
command: 04 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 05 00 00 00
command: 05 00 00 00
#
name: STOP_-
type: parsed
protocol: NECext
address: 05 00 00 00
command: 05 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 05 00 00 00
command: 06 00 00 00
#
name: DATE_-
type: parsed
protocol: NECext
address: 05 00 00 00
command: 06 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 05 00 00 00
command: 07 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 05 00 00 00
command: 08 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 05 00 00 00
command: 09 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 05 00 00 00
command: 0C 00 00 00
#
name: CHANNEL+
type: parsed
protocol: NECext
address: 05 00 00 00
command: 20 00 00 00
#
name: CHANNEL_-
type: parsed
protocol: NECext
address: 05 00 00 00
command: 21 00 00 00
#
name: PAUSE
type: parsed
protocol: NECext
address: 05 00 00 00
command: 29 00 00 00
#
name: REWIND_<<
type: parsed
protocol: NECext
address: 05 00 00 00
command: 32 00 00 00
#
name: FAST_FORWARD_>>
type: parsed
protocol: NECext
address: 05 00 00 00
command: 34 00 00 00
#
name: CURSOR_UP
type: parsed
protocol: NECext
address: 05 00 00 00
command: 35 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 05 00 00 00
command: 35 00 00 00
#
name: CURSOR_DOWN
type: parsed
protocol: NECext
address: 05 00 00 00
command: 36 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 05 00 00 00
command: 36 00 00 00
#
name: RECORD
type: parsed
protocol: NECext
address: 05 00 00 00
command: 37 00 00 00
#
name: PROGRAM
type: parsed
protocol: NECext
address: 05 00 00 00
command: 45 00 00 00
#
name: OK
type: parsed
protocol: NECext
address: 05 00 00 00
command: 57 00 00 00
