Filetype: IR signals file
Version: 1
# 
# Briloner Leuchten LED
#
name: ON
type: parsed
protocol: NEC
address: 00 00 00 00
command: 45 00 00 00
# 
name: OFF
type: parsed
protocol: NEC
address: 00 00 00 00
command: 47 00 00 00
