Filetype: IR signals file
Version: 1
# 
# Samsung TV Universal Remote BN59-01178W
# 
name: Tv_on/off
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 02 00 00 00
# 
name: Stb_on/off
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: E0 00 00 00
# 
name: Source
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 01 00 00 00
# 
name: 1
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 04 00 00 00
# 
name: 2
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 05 00 00 00
# 
name: 3
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 06 00 00 00
# 
name: 4
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 08 00 00 00
# 
name: 5
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 09 00 00 00
# 
name: 6
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 0A 00 00 00
# 
name: 7
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 0C 00 00 00
# 
name: 8
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 0D 00 00 00
# 
name: 9
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 0E 00 00 00
# 
name: 0
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 11 00 00 00
# 
name: Minus(-)
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 23 00 00 00
# 
name: Prev_ch
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 13 00 00 00
# 
name: Vol_up
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 07 00 00 00
# 
name: Vol_dn
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 0B 00 00 00
# 
name: Ch_next
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 12 00 00 00
# 
name: Ch_prev
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 10 00 00 00
# 
name: Mute
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 0F 00 00 00
# 
name: Ch_list
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 6B 00 00 00
# 
name: Menu
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 1A 00 00 00
# 
name: Smart_hub
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 79 00 00 00
# 
name: Guide
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 4F 00 00 00
# 
name: Tools
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 4B 00 00 00
# 
name: Info_(i)
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 1F 00 00 00
# 
name: Arrow_up
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 60 00 00 00
# 
name: Arrow_left
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 65 00 00 00
# 
name: Arrow_right
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 62 00 00 00
# 
name: Arrow_down
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 61 00 00 00
# 
name: Enter/middle
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 68 00 00 00
# 
name: Return/back
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 58 00 00 00
# 
name: Exit
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 2D 00 00 00
# 
name: A(red)
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 6C 00 00 00
# 
name: B(green)
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 14 00 00 00
# 
name: C(yellow)
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 15 00 00 00
# 
name: D(blue)
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 16 00 00 00
# 
name: E-manual
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 3F 00 00 00
# 
name: Search
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 73 00 00 00
# 
name: Keypad
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: D2 00 00 00
# 
name: P.size
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 3E 00 00 00
# 
name: Mts
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 00 00 00 00
# 
name: Cc
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 25 00 00 00
# 
name: Rewind
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 45 00 00 00
# 
name: Pause
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 4A 00 00 00
# 
name: Fast_forward
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 48 00 00 00
# 
name: Record
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 49 00 00 00
# 
name: Play
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 47 00 00 00
# 
name: Stop
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 46 00 00 00
