Filetype: IR signals file
Version: 1
# 
# Toshiba CT-9922 TV remote (tested with model: 14CJ1RS)
# 
name: Power
type: parsed
protocol: NEC
address: 40 00 00 00
command: 12 00 00 00
# 
name: Mute
type: parsed
protocol: NEC
address: 40 00 00 00
command: 10 00 00 00
# 
name: Vol_up
type: parsed
protocol: NEC
address: 40 00 00 00
command: 1A 00 00 00
# 
name: Vol_dn
type: parsed
protocol: NEC
address: 40 00 00 00
command: 1E 00 00 00
# 
name: Ch_next
type: parsed
protocol: NEC
address: 40 00 00 00
command: 1B 00 00 00
# 
name: Ch_prev
type: parsed
protocol: NEC
address: 40 00 00 00
command: 1F 00 00 00
# 
name: Menu
type: parsed
protocol: NEC
address: 40 00 00 00
command: 5B 00 00 00
# 
# TV/VIDEO select (->o)
name: Source
type: parsed
protocol: NEC
address: 40 00 00 00
command: 14 00 00 00
# 
name: Right
type: parsed
protocol: NEC
address: 40 00 00 00
command: 1A 00 00 00
# 
name: Left
type: parsed
protocol: NEC
address: 40 00 00 00
command: 1E 00 00 00
# 
name: Up
type: parsed
protocol: NEC
address: 40 00 00 00
command: 19 00 00 00
# 
name: Down
type: parsed
protocol: NEC
address: 40 00 00 00
command: 1D 00 00 00
#
# Picture control
name: Pic_cntrl
type: parsed
protocol: NEC
address: 40 00 00 00
command: 18 00 00 00
# 
# On-screen (call)
name: Info
type: parsed
protocol: NEC
address: 40 00 00 00
command: 16 00 00 00
# 
# Digit select (-/--)
name: Digit
type: parsed
protocol: NEC
address: 40 00 00 00
command: 0B 00 00 00
# 
name: 1
type: parsed
protocol: NEC
address: 40 00 00 00
command: 01 00 00 00
# 
name: 2
type: parsed
protocol: NEC
address: 40 00 00 00
command: 02 00 00 00
# 
name: 3
type: parsed
protocol: NEC
address: 40 00 00 00
command: 03 00 00 00
# 
name: 4
type: parsed
protocol: NEC
address: 40 00 00 00
command: 04 00 00 00
# 
name: 5
type: parsed
protocol: NEC
address: 40 00 00 00
command: 05 00 00 00
# 
name: 6
type: parsed
protocol: NEC
address: 40 00 00 00
command: 06 00 00 00
# 
name: 7
type: parsed
protocol: NEC
address: 40 00 00 00
command: 07 00 00 00
# 
name: 8
type: parsed
protocol: NEC
address: 40 00 00 00
command: 08 00 00 00
# 
name: 9
type: parsed
protocol: NEC
address: 40 00 00 00
command: 09 00 00 00
# 
name: 0
type: parsed
protocol: NEC
address: 40 00 00 00
command: 00 00 00 00
