Filetype: IR signals file
Version: 1
#
name: POWER
type: parsed
protocol: NECext
address: 00 BD 00 00
command: 01 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 00 BD 00 00
command: 04 00 00 00
#
name: TVVIDEO
type: parsed
protocol: NECext
address: 00 BD 00 00
command: 05 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 00 BD 00 00
command: 0A 00 00 00
#
name: RIGHT
type: parsed
protocol: NECext
address: 00 BD 00 00
command: 0C 00 00 00
#
name: LEFT
type: parsed
protocol: NECext
address: 00 BD 00 00
command: 10 00 00 00
#
name: PIP
type: parsed
protocol: NECext
address: 00 BD 00 00
command: 12 00 00 00
#
name: SLEEP
type: parsed
protocol: NECext
address: 00 BD 00 00
command: 13 00 00 00
#
name: WIDE
type: parsed
protocol: NECext
address: 00 BD 00 00
command: 14 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 00 BD 00 00
command: 15 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 00 BD 00 00
command: 16 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 00 BD 00 00
command: 17 00 00 00
#
name: UP
type: parsed
protocol: NECext
address: 00 BD 00 00
command: 18 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 00 BD 00 00
command: 19 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 00 BD 00 00
command: 1A 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 00 BD 00 00
command: 1B 00 00 00
#
name: DOWN
type: parsed
protocol: NECext
address: 00 BD 00 00
command: 1C 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 00 BD 00 00
command: 1D 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 00 BD 00 00
command: 1E 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 00 BD 00 00
command: 1F 00 00 00
#
name: INFO
type: parsed
protocol: NECext
address: 00 BD 00 00
command: 40 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 00 BD 00 00
command: 41 00 00 00
#
name: PRECH
type: parsed
protocol: NECext
address: 00 BD 00 00
command: 44 00 00 00
#
name: PC
type: parsed
protocol: NECext
address: 00 BD 00 00
command: 45 00 00 00
#
name: PLUSMINUS
type: parsed
protocol: NECext
address: 00 BD 00 00
command: 4B 00 00 00
