Filetype: IR signals file
Version: 1
#
name: pause/still
type: parsed
protocol: NECext
address: 16 00 00 00
command: 11 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 16 00 00 00
command: 12 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 16 00 00 00
command: 14 00 00 00
#
name: CHANNELUP
type: parsed
protocol: NECext
address: 16 00 00 00
command: 16 00 00 00
#
name: CH-
type: parsed
protocol: NECext
address: 16 00 00 00
command: 17 00 00 00
#
name: RECORD
type: parsed
protocol: NECext
address: 16 00 00 00
command: 18 00 00 00
#
name: REWIND
type: parsed
protocol: NECext
address: 16 00 00 00
command: 19 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 16 00 00 00
command: 1A 00 00 00
#
name: FORWARD
type: parsed
protocol: NECext
address: 16 00 00 00
command: 1B 00 00 00
