Filetype: IR signals file
Version: 1
#
name: 1
type: parsed
protocol: NECext
address: 02 00 00 00
command: 00 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 02 00 00 00
command: 01 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 02 00 00 00
command: 02 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 02 00 00 00
command: 04 00 00 00
#
name: KPMINUS
type: parsed
protocol: NECext
address: 02 00 00 00
command: 05 00 00 00
#
name: PAUSE
type: parsed
protocol: NECext
address: 02 00 00 00
command: 06 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 02 00 00 00
command: 09 00 00 00
#
name: TEXT
type: parsed
protocol: NECext
address: 02 00 00 00
command: 0A 00 00 00
#
name: UP
type: parsed
protocol: NECext
address: 02 00 00 00
command: 0B 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 02 00 00 00
command: 10 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 02 00 00 00
command: 12 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 02 00 00 00
command: 14 00 00 00
#
name: LEFT
type: parsed
protocol: NECext
address: 02 00 00 00
command: 1B 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 02 00 00 00
command: 1C 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 02 00 00 00
command: 20 00 00 00
#
name: FORWARD
type: parsed
protocol: NECext
address: 02 00 00 00
command: 21 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 02 00 00 00
command: 22 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 02 00 00 00
command: 24 00 00 00
#
name: Switch
type: parsed
protocol: NECext
address: 02 00 00 00
command: 25 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 02 00 00 00
command: 26 00 00 00
#
name: Input
type: parsed
protocol: NECext
address: 02 00 00 00
command: 27 00 00 00
#
name: RECORD
type: parsed
protocol: NECext
address: 02 00 00 00
command: 2A 00 00 00
#
name: DOWN
type: parsed
protocol: NECext
address: 02 00 00 00
command: 2B 00 00 00
#
name: QUIT
type: parsed
protocol: NECext
address: 02 00 00 00
command: 2E 00 00 00
#
name: INFO
type: parsed
protocol: NECext
address: 02 00 00 00
command: 2F 00 00 00
#
name: Okay
type: parsed
protocol: NECext
address: 02 00 00 00
command: 33 00 00 00
#
name: Blank
type: parsed
protocol: NECext
address: 02 00 00 00
command: 36 00 00 00
#
name: KPPLUS
type: parsed
protocol: NECext
address: 02 00 00 00
command: 39 00 00 00
#
name: RIGHT
type: parsed
protocol: NECext
address: 02 00 00 00
command: 3B 00 00 00
#
name: REWIND
type: parsed
protocol: NECext
address: 02 00 00 00
command: 3E 00 00 00
