Filetype: IR signals file
Version: 1
# 
# TCL TS5010 Soundbar
#
name: Power
type: parsed
protocol: NECext
address: 86 FF 00 00
command: 1C E3 00 00
# 
name: Vol_up
type: parsed
protocol: NECext
address: 86 FF 00 00
command: 21 DE 00 00
# 
name: Vol_dn
type: parsed
protocol: NECext
address: 86 FF 00 00
command: 2B D4 00 00
# 
name: VolMute
type: parsed
protocol: NECext
address: 86 FF 00 00
command: 1D E2 00 00
# 
name: Ch_next
type: parsed
protocol: NECext
address: 86 FF 00 00
command: 21 DE 00 00
# 
name: Ch_prev
type: parsed
protocol: NECext
address: 86 FF 00 00
command: 2B D4 00 00
# 
name: DPad_Up
type: parsed
protocol: NECext
address: 86 FF 00 00
command: 21 DE 00 00
# 
name: DPad_Down
type: parsed
protocol: NECext
address: 86 FF 00 00
command: 2B D4 00 00
# 
name: DPad_Left
type: parsed
protocol: NECext
address: 86 FF 00 00
command: 13 EC 00 00
# 
name: DPad_Right
type: parsed
protocol: NECext
address: 86 FF 00 00
command: 14 EB 00 00
# 
name: Rewind
type: parsed
protocol: NECext
address: 86 FF 00 00
command: 13 EC 00 00
# 
name: Play
type: parsed
protocol: NECext
address: 86 FF 00 00
command: 2A D5 00 00
# 
name: FastForward
type: parsed
protocol: NECext
address: 86 FF 00 00
command: 14 EB 00 00
# 
name: Pause
type: parsed
protocol: NECext
address: 86 FF 00 00
command: 2A D5 00 00
# 
name: Stop
type: parsed
protocol: NECext
address: 86 FF 00 00
command: 2A D5 00 00
# 
name: Skip_Back
type: parsed
protocol: NECext
address: 86 FF 00 00
command: 13 EC 00 00
# 
name: Skip_Forward
type: parsed
protocol: NECext
address: 86 FF 00 00
command: 14 EB 00 00
# 
name: Guide
type: parsed
protocol: NECext
address: 86 FF 00 00
command: 2A D5 00 00
# 
name: Info
type: parsed
protocol: NECext
address: 86 FF 00 00
command: 2B D4 00 00
# 
name: InputAux
type: parsed
protocol: NECext
address: 86 FF 00 00
command: 10 EF 00 00
# 
name: InputBluetooth
type: parsed
protocol: NECext
address: 86 FF 00 00
command: 1B E4 00 00
# 
name: InputOptical
type: parsed
protocol: NECext
address: 86 FF 00 00
command: 12 ED 00 00
# 
name: InputUSB
type: parsed
protocol: NECext
address: 86 FF 00 00
command: 29 D6 00 00
# 
name: Movie
type: parsed
protocol: NECext
address: 86 FF 00 00
command: 2C D3 00 00
# 
name: Music
type: parsed
protocol: NECext
address: 86 FF 00 00
command: 27 D8 00 00
# 
name: News
type: parsed
protocol: NECext
address: 86 FF 00 00
command: 2D D2 00 00
# 
name: Pair
type: parsed
protocol: NECext
address: 86 FF 00 00
command: 2A D5 00 00
