Filetype: IR signals file
Version: 1
#
# XORO HSD-303
# Autogenerated from ircodes/XORO/HSD-303.xml
#
name: SLEEP
type: parsed
protocol: NECext
address: FF 00 00 00
command: 27 D8 00 00
#
name: OSD
type: parsed
protocol: NECext
address: FF 00 00 00
command: A7 58 00 00
#
name: PBC
type: parsed
protocol: NECext
address: FF 00 00 00
command: E5 1A 00 00
#
name: EJECT
type: parsed
protocol: NECext
address: FF 00 00 00
command: 65 9A 00 00
#
name: A-B
type: parsed
protocol: NECext
address: FF 00 00 00
command: 37 C8 00 00
#
name: SUBTITLE
type: parsed
protocol: NECext
address: FF 00 00 00
command: 2F D0 00 00
#
name: ANGLE
type: parsed
protocol: NECext
address: FF 00 00 00
command: 17 E8 00 00
#
name: TRACK
type: parsed
protocol: NECext
address: FF 00 00 00
command: 07 F8 00 00
#
name: 1
type: parsed
protocol: NECext
address: FF 00 00 00
command: B7 48 00 00
#
name: 2
type: parsed
protocol: NECext
address: FF 00 00 00
command: F5 0A 00 00
#
name: 3
type: parsed
protocol: NECext
address: FF 00 00 00
command: 75 8A 00 00
#
name: 4
type: parsed
protocol: NECext
address: FF 00 00 00
command: AF 50 00 00
#
name: 5
type: parsed
protocol: NECext
address: FF 00 00 00
command: ED 12 00 00
#
name: 6
type: parsed
protocol: NECext
address: FF 00 00 00
command: 6D 92 00 00
#
name: 7
type: parsed
protocol: NECext
address: FF 00 00 00
command: 97 68 00 00
#
name: 8
type: parsed
protocol: NECext
address: FF 00 00 00
command: D5 2A 00 00
#
name: 9
type: parsed
protocol: NECext
address: FF 00 00 00
command: 55 AA 00 00
#
name: GOTO
type: parsed
protocol: NECext
address: FF 00 00 00
command: 45 BA 00 00
#
name: 0
type: parsed
protocol: NECext
address: FF 00 00 00
command: 87 78 00 00
#
name: 10+
type: parsed
protocol: NECext
address: FF 00 00 00
command: C5 3A 00 00
#
name: ITEM
type: parsed
protocol: NECext
address: FF 00 00 00
command: 47 B8 00 00
#
name: Unknown
type: parsed
protocol: NECext
address: FF 00 00 00
command: C7 38 00 00
#
name: PROGRAM
type: parsed
protocol: NECext
address: FF 00 00 00
command: 05 FA 00 00
#
name: Unknown
type: parsed
protocol: NECext
address: FF 00 00 00
command: 67 98 00 00
#
name: ENTER
type: parsed
protocol: NECext
address: FF 00 00 00
command: E7 18 00 00
#
name: Unknown
type: parsed
protocol: NECext
address: FF 00 00 00
command: 25 DA 00 00
#
name: V-MODEL
type: parsed
protocol: NECext
address: FF 00 00 00
command: 77 88 00 00
#
name: Unknown
type: parsed
protocol: NECext
address: FF 00 00 00
command: D7 28 00 00
#
name: MENU
type: parsed
protocol: NECext
address: FF 00 00 00
command: 57 A8 00 00
#
name: ZOOM
type: parsed
protocol: NECext
address: FF 00 00 00
command: F7 08 00 00
#
name: REPEAT
type: parsed
protocol: NECext
address: FF 00 00 00
command: 35 CA 00 00
#
name: SETUP
type: parsed
protocol: NECext
address: FF 00 00 00
command: 15 EA 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: FF 00 00 00
command: 4F B0 00 00
#
name: Unknown
type: parsed
protocol: NECext
address: FF 00 00 00
command: 6F 90 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: FF 00 00 00
command: CF 30 00 00
#
name: Unknown
type: parsed
protocol: NECext
address: FF 00 00 00
command: 8D 72 00 00
#
name: CHANNEL
type: parsed
protocol: NECext
address: FF 00 00 00
command: EF 10 00 00
#
name: FWD
type: parsed
protocol: NECext
address: FF 00 00 00
command: 0D F2 00 00
#
name: PREV
type: parsed
protocol: NECext
address: FF 00 00 00
command: AD 52 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: FF 00 00 00
command: 1D E2 00 00
#
name: NEXT
type: parsed
protocol: NECext
address: FF 00 00 00
command: 2D D2 00 00
#
name: PAUSE
type: parsed
protocol: NECext
address: FF 00 00 00
command: 5F A0 00 00
#
name: STOP
type: parsed
protocol: NECext
address: FF 00 00 00
command: DF 20 00 00
#
name: RESUME
type: parsed
protocol: NECext
address: FF 00 00 00
command: 7F 80 00 00
#
name: SHUFFLE
type: parsed
protocol: NECext
address: FF 00 00 00
command: FF 00 00 00
#
name: STEP
type: parsed
protocol: NECext
address: FF 00 00 00
command: BD 42 00 00
#
name: SLOW
type: parsed
protocol: NECext
address: FF 00 00 00
command: 3D C2 00 00
