Filetype: IR signals file
Version: 1
#
# Yamaha generic audio receivers and amplifiers.
# The remote model is RAS5 / WV50010, it has buttons
# for controlling receivers, tuners and players.
#
# Tested with Yamaha A-S500.
#
name: Power
type: parsed
protocol: NECext
address: 7E 81 00 00
command: 2A D4 00 00
# 
name: Vol_up
type: parsed
protocol: NECext
address: 7A 85 00 00
command: 1A E4 00 00
# 
name: Vol_dn
type: parsed
protocol: NECext
address: 7A 85 00 00
command: 1B E5 00 00
# 
name: Mute
type: parsed
protocol: NECext
address: 7A 85 00 00
command: 1C E2 00 00
# 
name: CD
type: parsed
protocol: NECext
address: 7A 85 00 00
command: 15 EB 00 00
# 
name: Tuner
type: parsed
protocol: NECext
address: 7A 85 00 00
command: 16 E8 00 00
# 
name: Line1
type: parsed
protocol: NECext
address: 7A 85 00 00
command: C1 3F 00 00
# 
name: Line2
type: parsed
protocol: NECext
address: 7A 85 00 00
command: 18 E6 00 00
# 
name: Line3
type: parsed
protocol: NECext
address: 7A 85 00 00
command: 19 E7 00 00
# 
name: Phono
type: parsed
protocol: NECext
address: 7A 85 00 00
command: 14 EA 00 00
# 
name: Dock
type: parsed
protocol: NECext
address: 7F 01 00 00
command: 4A B4 00 00
