Filetype: IR signals file
Version: 1
#
name: 0
type: parsed
protocol: NECext
address: A2 00 00 00
command: 00 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: A2 00 00 00
command: 01 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: A2 00 00 00
command: 02 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: A2 00 00 00
command: 03 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: A2 00 00 00
command: 04 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: A2 00 00 00
command: 05 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: A2 00 00 00
command: 06 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: A2 00 00 00
command: 07 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: A2 00 00 00
command: 08 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: A2 00 00 00
command: 09 00 00 00
#
name: out+
type: parsed
protocol: NECext
address: A2 00 00 00
command: 0A 00 00 00
#
name: out-
type: parsed
protocol: NECext
address: A2 00 00 00
command: 0B 00 00 00
#
name: pgm
type: parsed
protocol: NECext
address: A2 00 00 00
command: 0D 00 00 00
#
name: for
type: parsed
protocol: NECext
address: A2 00 00 00
command: 0E 00 00 00
#
name: rev
type: parsed
protocol: NECext
address: A2 00 00 00
command: 0F 00 00 00
#
name: NEXT
type: parsed
protocol: NECext
address: A2 00 00 00
command: 10 00 00 00
#
name: BACK
type: parsed
protocol: NECext
address: A2 00 00 00
command: 11 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: A2 00 00 00
command: 16 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: A2 00 00 00
command: 17 00 00 00
#
name: PAUSE
type: parsed
protocol: NECext
address: A2 00 00 00
command: 18 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: A2 00 00 00
command: 1C 00 00 00
#
name: rnd
type: parsed
protocol: NECext
address: A2 00 00 00
command: 4A 00 00 00
#
name: >10
type: parsed
protocol: NECext
address: A2 00 00 00
command: 56 00 00 00
#
name: hi-lite
type: parsed
protocol: NECext
address: A2 00 00 00
command: 5E 00 00 00
