Filetype: IR signals file
Version: 1
#
name: 0
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 00 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 01 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 02 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 03 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 04 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 05 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 06 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 07 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 08 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 09 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 0A 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 0B 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 0C 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 10 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 11 00 00 00
#
name: CHANNELUP
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 12 00 00 00
#
name: CHANNELDOWN
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 13 00 00 00
#
name: CYCLEWINDOWS
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 1E 00 00 00
#
name: TEXT
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 21 00 00 00
#
name: OK
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 25 00 00 00
#
name: UP
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 26 00 00 00
#
name: DOWN
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 27 00 00 00
#
name: LEFT
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 28 00 00 00
#
name: RIGHT
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 29 00 00 00
#
name: pre-ch
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 2A 00 00 00
#
name: pip
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 2B 00 00 00
#
name: SLEEP
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 2C 00 00 00
#
name: VIDEO
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 30 00 00 00
#
name: scart
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 31 00 00 00
#
name: PC
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 32 00 00 00
#
name: dtvmenu
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 33 00 00 00
#
name: ZOOMOUT
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 34 00 00 00
#
name: mix
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 35 00 00 00
#
name: INFO
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 36 00 00 00
#
name: SUBTITLE
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 37 00 00 00
#
name: TV
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 40 00 00 00
#
name: RED
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 45 00 00 00
#
name: GREEN
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 46 00 00 00
#
name: BLUE
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 47 00 00 00
#
name: YELLOW
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 49 00 00 00
#
name: display
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 70 00 00 00
#
name: EXIT
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 71 00 00 00
#
name: SUBTITLE
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 72 00 00 00
#
name: index
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 73 00 00 00
#
name: sound
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 74 00 00 00
#
name: ZOOMIN
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 79 00 00 00
#
name: size
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 86 00 00 00
#
name: reveal
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 87 00 00 00
#
name: hold
type: parsed
protocol: NECext
address: 83 F1 00 00
command: 88 00 00 00
