Filetype: IR signals file
Version: 1
#
name: 0
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 00 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 01 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 02 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 03 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 04 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 05 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 06 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 07 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 08 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 09 00 00 00
#
name: INFO
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 0A 00 00 00
#
name: RED
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 0B 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 0D 00 00 00
#
name: ENTER
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 0E 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 0F 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 10 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 11 00 00 00
#
name: AGAIN
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 12 00 00 00
#
name: UpArrow
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 14 00 00 00
#
name: DownArrow
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 15 00 00 00
#
name: LeftArrow
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 16 00 00 00
#
name: RightArrow
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 17 00 00 00
#
name: INFO
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 1B 00 00 00
#
name: SkipForward
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 1E 00 00 00
#
name: EXIT
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 1F 00 00 00
#
name: CHANNELUP
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 20 00 00 00
#
name: CHANNELDOWN
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 21 00 00 00
#
name: REWIND
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 24 00 00 00
#
name: OK
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 25 00 00 00
#
name: BLUE
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 29 00 00 00
#
name: GREEN
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 2E 00 00 00
#
name: PAUSE
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 30 00 00 00
#
name: REWIND
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 32 00 00 00
#
name: FASTFORWARD
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 34 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 35 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 36 00 00 00
#
name: RECORD
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 37 00 00 00
#
name: YELLOW
type: parsed
protocol: NECext
address: 1E 00 00 00
command: 38 00 00 00
