Filetype: IR signals file
Version: 1
# 
# For Vitec (Exterity) IPTV
# 
name: Power
type: parsed
protocol: NECext
address: AD ED 00 00
command: B5 4A 00 00
# 
name: Tv
type: parsed
protocol: NECext
address: AD ED 00 00
command: C9 36 00 00
# 
name: Home
type: parsed
protocol: NECext
address: AD ED 00 00
command: CA 35 00 00
# 
name: Guide
type: parsed
protocol: NECext
address: AD ED 00 00
command: CB 34 00 00
# 
name: Text
type: parsed
protocol: NECext
address: AD ED 00 00
command: AB 54 00 00
# 
name: Vol_up
type: parsed
protocol: NECext
address: AD ED 00 00
command: BA 45 00 00
# 
name: Vol_dn
type: parsed
protocol: NECext
address: AD ED 00 00
command: BB 44 00 00
# 
name: Ch_next
type: parsed
protocol: NECext
address: AD ED 00 00
command: B0 4F 00 00
# 
name: Ch_prev
type: parsed
protocol: NECext
address: AD ED 00 00
command: B1 4E 00 00
# 
name: Mute
type: parsed
protocol: NECext
address: AD ED 00 00
command: C5 3A 00 00
# 
name: Menu
type: parsed
protocol: NECext
address: AD ED 00 00
command: A5 5A 00 00
# 
name: Up
type: parsed
protocol: NECext
address: AD ED 00 00
command: B2 4D 00 00
# 
name: Down
type: parsed
protocol: NECext
address: AD ED 00 00
command: B4 4B 00 00
# 
name: Left
type: parsed
protocol: NECext
address: AD ED 00 00
command: A9 56 00 00
# 
name: Right
type: parsed
protocol: NECext
address: AD ED 00 00
command: BD 42 00 00
# 
name: Ok
type: parsed
protocol: NECext
address: AD ED 00 00
command: B3 4C 00 00
