Filetype: IR signals file
Version: 1
#
name: CURSOR_UP
type: parsed
protocol: NECext
address: 73 00 00 00
command: 01 00 00 00
#
name: MENU_UP
type: parsed
protocol: NECext
address: 73 00 00 00
command: 01 00 00 00
#
name: CURSOR_DOWN
type: parsed
protocol: NECext
address: 73 00 00 00
command: 02 00 00 00
#
name: MENU_DOWN
type: parsed
protocol: NECext
address: 73 00 00 00
command: 02 00 00 00
#
name: EXIT
type: parsed
protocol: NECext
address: 73 00 00 00
command: 03 00 00 00
#
name: POWER_ON
type: parsed
protocol: NECext
address: 73 00 00 00
command: 05 00 00 00
#
name: POWER_OFF
type: parsed
protocol: NECext
address: 73 00 00 00
command: 06 00 00 00
#
name: HIDE
type: parsed
protocol: NECext
address: 73 00 00 00
command: 1D 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 73 00 00 00
command: 2E 00 00 00
#
name: ENTER
type: parsed
protocol: NECext
address: 73 00 00 00
command: 2F 00 00 00
#
name: CURSOR_RIGHT
type: parsed
protocol: NECext
address: 73 00 00 00
command: 34 00 00 00
#
name: MENU_RIGHT
type: parsed
protocol: NECext
address: 73 00 00 00
command: 34 00 00 00
#
name: CURSOR_LEFT
type: parsed
protocol: NECext
address: 73 00 00 00
command: 36 00 00 00
#
name: MENU_LEFT
type: parsed
protocol: NECext
address: 73 00 00 00
command: 36 00 00 00
#
name: INPUT:_VIDEO
type: parsed
protocol: NECext
address: 73 00 00 00
command: 4B 00 00 00
#
name: VIDEO
type: parsed
protocol: NECext
address: 73 00 00 00
command: 4B 00 00 00
#
name: INPUT:_S-VIDEO
type: parsed
protocol: NECext
address: 73 00 00 00
command: 4C 00 00 00
#
name: S-VIDEO
type: parsed
protocol: NECext
address: 73 00 00 00
command: 4C 00 00 00
#
name: INPUT:_COMPONENT
type: parsed
protocol: NECext
address: 73 00 00 00
command: 4D 00 00 00
#
name: COMPONENT
type: parsed
protocol: NECext
address: 73 00 00 00
command: 4D 00 00 00
#
name: TEST
type: parsed
protocol: NECext
address: 73 00 00 00
command: 59 00 00 00
#
name: IMAGE:_CINEMA
type: parsed
protocol: NECext
address: 73 00 00 00
command: 69 00 00 00
#
name: CINEMA
type: parsed
protocol: NECext
address: 73 00 00 00
command: 69 00 00 00
#
name: IMAGE:_NATURAL
type: parsed
protocol: NECext
address: 73 00 00 00
command: 6A 00 00 00
#
name: NATURAL
type: parsed
protocol: NECext
address: 73 00 00 00
command: 6A 00 00 00
#
name: IMAGE:_DYNAMIC
type: parsed
protocol: NECext
address: 73 00 00 00
command: 6B 00 00 00
#
name: DYNAMIC
type: parsed
protocol: NECext
address: 73 00 00 00
command: 6B 00 00 00
#
name: IMAGE:_USER_1
type: parsed
protocol: NECext
address: 73 00 00 00
command: 6C 00 00 00
#
name: USER_1
type: parsed
protocol: NECext
address: 73 00 00 00
command: 6C 00 00 00
#
name: IMAGE:_USER_2
type: parsed
protocol: NECext
address: 73 00 00 00
command: 6D 00 00 00
#
name: USER_2
type: parsed
protocol: NECext
address: 73 00 00 00
command: 6D 00 00 00
#
name: IMAGE:_USER_3
type: parsed
protocol: NECext
address: 73 00 00 00
command: 6E 00 00 00
#
name: USER_3
type: parsed
protocol: NECext
address: 73 00 00 00
command: 6E 00 00 00
#
name: INPUT:_HDMI_1
type: parsed
protocol: NECext
address: 73 00 00 00
command: 70 00 00 00
#
name: HDMI_1
type: parsed
protocol: NECext
address: 73 00 00 00
command: 70 00 00 00
#
name: INPUT:_HDMI_2
type: parsed
protocol: NECext
address: 73 00 00 00
command: 71 00 00 00
#
name: HDMI_2
type: parsed
protocol: NECext
address: 73 00 00 00
command: 71 00 00 00
#
name: INFO
type: parsed
protocol: NECext
address: 73 00 00 00
command: 74 00 00 00
#
name: GAMMA
type: parsed
protocol: NECext
address: 73 00 00 00
command: 75 00 00 00
#
name: COLOR_TEMP
type: parsed
protocol: NECext
address: 73 00 00 00
command: 76 00 00 00
#
name: ASPECT
type: parsed
protocol: NECext
address: 73 00 00 00
command: 77 00 00 00
#
name: CONTRAST_+
type: parsed
protocol: NECext
address: 73 00 00 00
command: 78 00 00 00
#
name: CONTRAST_-
type: parsed
protocol: NECext
address: 73 00 00 00
command: 79 00 00 00
#
name: BRIGHTNESS_+
type: parsed
protocol: NECext
address: 73 00 00 00
command: 7A 00 00 00
#
name: BRIGHT_+
type: parsed
protocol: NECext
address: 73 00 00 00
command: 7A 00 00 00
#
name: BRIGHTNESS_-
type: parsed
protocol: NECext
address: 73 00 00 00
command: 7B 00 00 00
#
name: BRIGHT_-
type: parsed
protocol: NECext
address: 73 00 00 00
command: 7B 00 00 00
#
name: COLOR_+
type: parsed
protocol: NECext
address: 73 00 00 00
command: 7C 00 00 00
#
name: COLOR_-
type: parsed
protocol: NECext
address: 73 00 00 00
command: 7D 00 00 00
#
name: SHARPNESS_+
type: parsed
protocol: NECext
address: 73 00 00 00
command: 7E 00 00 00
#
name: SHARP_+
type: parsed
protocol: NECext
address: 73 00 00 00
command: 7E 00 00 00
#
name: SHARPNESS_-
type: parsed
protocol: NECext
address: 73 00 00 00
command: 7F 00 00 00
#
name: SHARP_-
type: parsed
protocol: NECext
address: 73 00 00 00
command: 7F 00 00 00
