Filetype: IR signals file
Version: 1
# 
# Craig Electronics Speaker CHT904
#  
name: Power
type: parsed
protocol: NEC
address: 20 00 00 00
command: 09 00 00 00
# 
name: Vol_up
type: parsed
protocol: NEC
address: 20 00 00 00
command: 0E 00 00 00
# 
name: Vol_dn
type: parsed
protocol: NEC
address: 20 00 00 00
command: 1A 00 00 00
# 
name: VolumeMute
type: parsed
protocol: NEC
address: 20 00 00 00
command: 1F 00 00 00
# 
name: Ch_next
type: parsed
protocol: NEC
address: 20 00 00 00
command: 11 00 00 00
# 
name: Ch_prev
type: parsed
protocol: NEC
address: 20 00 00 00
command: 01 00 00 00
# 
name: ChUp_2
type: parsed
protocol: NEC
address: 20 00 00 00
command: 17 00 00 00
# 
name: ChDown_2
type: parsed
protocol: NEC
address: 20 00 00 00
command: 0F 00 00 00
# 
name: Auto
type: parsed
protocol: NEC
address: 20 00 00 00
command: 15 00 00 00
# 
name: InputNext
type: parsed
protocol: NEC
address: 20 00 00 00
command: 0D 00 00 00
# 
name: Reset
type: parsed
protocol: NEC
address: 20 00 00 00
command: 1B 00 00 00
# 
name: SRS
type: parsed
protocol: NEC
address: 20 00 00 00
command: 1D 00 00 00
# 
name: Stereo
type: parsed
protocol: NEC
address: 20 00 00 00
command: 12 00 00 00
# 
name: SubUp
type: parsed
protocol: NEC
address: 20 00 00 00
command: 00 00 00 00
# 
name: SubDown
type: parsed
protocol: NEC
address: 20 00 00 00
command: 03 00 00 00
