Filetype: IR signals file
Version: 1
#
name: POWER
type: parsed
protocol: NECext
address: 00 00 00 00
command: 00 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 00 00 00 00
command: 01 00 00 00
#
name: OK
type: parsed
protocol: NECext
address: 00 00 00 00
command: 02 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 00 00 00 00
command: 03 00 00 00
#
name: LANGUAGE
type: parsed
protocol: NECext
address: 00 00 00 00
command: 04 00 00 00
#
name: CHANNELUP
type: parsed
protocol: NECext
address: 00 00 00 00
command: 05 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 00 00 00 00
command: 06 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 00 00 00 00
command: 07 00 00 00
#
name: SEARCH
type: parsed
protocol: NECext
address: 00 00 00 00
command: 08 00 00 00
#
name: EXIT
type: parsed
protocol: NECext
address: 00 00 00 00
command: 09 00 00 00
#
name: CHANNELDOWN
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0A 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0B 00 00 00
#
name: Memory
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0C 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0E 00 00 00
#
name: TV/Radio
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0F 00 00 00
#
name: FAVORITES
type: parsed
protocol: NECext
address: 00 00 00 00
command: 10 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 00 00 00 00
command: 11 00 00 00
#
name: AUDIO
type: parsed
protocol: NECext
address: 00 00 00 00
command: 12 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 00 00 00 00
command: 13 00 00 00
#
name: GuideUp
type: parsed
protocol: NECext
address: 00 00 00 00
command: 14 00 00 00
#
name: INFO
type: parsed
protocol: NECext
address: 00 00 00 00
command: 15 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 00 00 00 00
command: 16 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 00 00 00 00
command: 17 00 00 00
#
name: GuideDown
type: parsed
protocol: NECext
address: 00 00 00 00
command: 18 00 00 00
#
name: TEXT
type: parsed
protocol: NECext
address: 00 00 00 00
command: 19 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 00 00 00 00
command: 1A 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 00 00 00 00
command: 1B 00 00 00
#
name: INFO
type: parsed
protocol: NECext
address: 00 00 00 00
command: 1C 00 00 00
#
name: PRList
type: parsed
protocol: NECext
address: 00 00 00 00
command: 1D 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 00 00 00 00
command: 1E 00 00 00
#
name: PAUSE
type: parsed
protocol: NECext
address: 00 00 00 00
command: 1F 00 00 00
#
name: SLEEP
type: parsed
protocol: NECext
address: 00 00 00 00
command: 40 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 00 00 00 00
command: 44 00 00 00
#
name: P/N
type: parsed
protocol: NECext
address: 00 00 00 00
command: 48 00 00 00
#
name: Spiral
type: parsed
protocol: NECext
address: 00 00 00 00
command: 4C 00 00 00
#
name: TV/AV
type: parsed
protocol: NECext
address: 00 00 00 00
command: 50 00 00 00
#
name: KPMINUS
type: parsed
protocol: NECext
address: 00 00 00 00
command: 54 00 00 00
#
name: KPPLUS
type: parsed
protocol: NECext
address: 00 00 00 00
command: 58 00 00 00
#
name: MODE
type: parsed
protocol: NECext
address: 00 00 00 00
command: 5C 00 00 00
