Filetype: IR signals file
Version: 1
#
name: POWER
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 00 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 01 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 02 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 03 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 04 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 05 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 06 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 07 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 08 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 09 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 0A 00 00 00
#
name: 10CHANNELSUP
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 0B 00 00 00
#
name: s7
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 0C 00 00 00
#
name: s8
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 0E 00 00 00
#
name: s9
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 11 00 00 00
#
name: fmmode
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 12 00 00 00
#
name: s6
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 14 00 00 00
#
name: s1
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 15 00 00 00
#
name: s2
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 16 00 00 00
#
name: s4
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 17 00 00 00
#
name: s5
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 19 00 00 00
#
name: band
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 1C 00 00 00
#
name: func
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 1E 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 40 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 41 00 00 00
#
name: FORWARD
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 42 00 00 00
#
name: UP
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 42 00 00 00
#
name: bwd
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 43 00 00 00
#
name: DOWN
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 43 00 00 00
#
name: PAUSE
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 44 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 4D 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 4E 00 00 00
#
name: s+10
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 50 00 00 00
#
name: ddp1
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 51 00 00 00
#
name: ddp2
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 52 00 00 00
#
name: ddp3
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 53 00 00 00
#
name: s3
type: parsed
protocol: NECext
address: 6E 00 00 00
command: 56 00 00 00
