Filetype: IR signals file
Version: 1
#
name: STOP
type: parsed
protocol: NECext
address: A3 00 00 00
command: 98 00 00 00
#
name: CURSOR_DOWN
type: parsed
protocol: NECext
address: A3 00 00 00
command: 98 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: A3 00 00 00
command: 98 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: Unknown
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: +10
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: ANGLE
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: AUDIO
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: CLEAR
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: CONDITION_MEMORY
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: DISPLAY
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: DOWN
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: ENTER
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: LAST_MEMORY
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: LEFT
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: OPEN/CLOSE
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: PROGRAM
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: RANDOM
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: REPEAT
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: REPEAT_A-B
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: RETURN
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: RIGHT
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: SEARCH_MODE
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: SET_UP
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: SLOW_MOTION_-
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: SLOW_MOTION_+
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: SUB_TITLE
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: TOP_MENU
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: UP
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: ANGLE
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: Unknown
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: ASPECT
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: AUDIO_MODE
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: CHAPTER/TIME
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: DISPLAY
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: RETURN
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: STEP<<
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: STEP>>
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: SUBTITLE
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: TITLE
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: +10
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: A-B
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: CLEAR
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: CONDITION_MEMORY
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: CURSOR_DOWN
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: CURSOR_LEFT
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: CURSOR_RIGHT
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: CURSOR_UP
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: ENTER
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: LAST_MEMORY
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: OPEN/CLOSE
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: PROGRAM
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: RANDOM
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: REPEAT
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: SEARCH_MODE
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: SETUP
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: SLOW_-
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: SLOW_+
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: TOP_MENU
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: CHP/TIME
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: CONDITION
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: DISC_SIDE
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: LAST_MEMO
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: MODE
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: SIDE_A/B
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: AUDIO
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: DOWNV
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: LEFT<
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: RIGHT>
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: STEP<
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: STEP>
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: UP^
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: POWER_OFF
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: POWER_ON
type: parsed
protocol: NECext
address: A3 00 00 00
command: 99 00 00 00
#
name: FORWARD
type: parsed
protocol: NECext
address: A3 00 00 00
command: 9A 00 00 00
#
name: CURSOR_RIGHT
type: parsed
protocol: NECext
address: A3 00 00 00
command: 9A 00 00 00
#
name: SCAN_>>
type: parsed
protocol: NECext
address: A3 00 00 00
command: 9A 00 00 00
#
name: SKIP_>>
type: parsed
protocol: NECext
address: A3 00 00 00
command: 9A 00 00 00
#
name: FRAME_>>
type: parsed
protocol: NECext
address: A3 00 00 00
command: 9A 00 00 00
#
name: SEARCH_>>
type: parsed
protocol: NECext
address: A3 00 00 00
command: 9A 00 00 00
#
name: REVERSE
type: parsed
protocol: NECext
address: A3 00 00 00
command: 9B 00 00 00
#
name: CURSOR_LEFT
type: parsed
protocol: NECext
address: A3 00 00 00
command: 9B 00 00 00
#
name: SCAN_<<
type: parsed
protocol: NECext
address: A3 00 00 00
command: 9B 00 00 00
#
name: SKIP_<<
type: parsed
protocol: NECext
address: A3 00 00 00
command: 9B 00 00 00
#
name: FRAME_<<
type: parsed
protocol: NECext
address: A3 00 00 00
command: 9B 00 00 00
#
name: SEARCH_<<
type: parsed
protocol: NECext
address: A3 00 00 00
command: 9B 00 00 00
#
name: NEXT
type: parsed
protocol: NECext
address: A3 00 00 00
command: 9C 00 00 00
#
name: SKIP_>>
type: parsed
protocol: NECext
address: A3 00 00 00
command: 9C 00 00 00
#
name: NEXT_>>
type: parsed
protocol: NECext
address: A3 00 00 00
command: 9C 00 00 00
#
name: NEXT
type: parsed
protocol: NECext
address: A3 00 00 00
command: 9C 00 00 00
#
name: TRACK>
type: parsed
protocol: NECext
address: A3 00 00 00
command: 9C 00 00 00
#
name: PREVIOUS
type: parsed
protocol: NECext
address: A3 00 00 00
command: 9D 00 00 00
#
name: SKIP_<<
type: parsed
protocol: NECext
address: A3 00 00 00
command: 9D 00 00 00
#
name: PREVIOUS_<<
type: parsed
protocol: NECext
address: A3 00 00 00
command: 9D 00 00 00
#
name: PREV
type: parsed
protocol: NECext
address: A3 00 00 00
command: 9D 00 00 00
#
name: TRACK<
type: parsed
protocol: NECext
address: A3 00 00 00
command: 9D 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: A3 00 00 00
command: 9E 00 00 00
#
name: ENTER
type: parsed
protocol: NECext
address: A3 00 00 00
command: 9E 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: A3 00 00 00
command: 9E 00 00 00
#
name: PAUSE
type: parsed
protocol: NECext
address: A3 00 00 00
command: 9F 00 00 00
#
name: CURSOR_UP
type: parsed
protocol: NECext
address: A3 00 00 00
command: 9F 00 00 00
#
name: PAUSE
type: parsed
protocol: NECext
address: A3 00 00 00
command: 9F 00 00 00
